(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.0044)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Glider")
		(date "2025-09-09")
		(rev "R1.3")
	)
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" power)
		(2 "In2.Cu" mixed)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.025)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.127)
				(material "FR4")
				(epsilon_r 4.2)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0152)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.6)
				(material "FR4")
				(epsilon_r 4.2)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0152)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.127)
				(material "FR4")
				(epsilon_r 4.2)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.025)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 68.5 106.5)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(U5-SW)")
	(net 2 "Net-(U5-BS)")
	(net 3 "+5V_EPD")
	(net 4 "+DRAM_VREF")
	(net 5 "EPDC_GDOE")
	(net 6 "EPDC_GDCLK")
	(net 7 "EPDC_GDSP")
	(net 8 "EPDC_SDCE0")
	(net 9 "/fpga_ddr/DRAM_CKP")
	(net 10 "/fpga_ddr/DRAM_CKN")
	(net 11 "Net-(U28-SW)")
	(net 12 "Net-(U28-BS)")
	(net 13 "Net-(U28-FB)")
	(net 14 "EPDC_SDLE")
	(net 15 "EPDC_SDOE")
	(net 16 "/fpga_ddr/DRAM_ADDR14")
	(net 17 "/fpga_ddr/DRAM_ADDR10")
	(net 18 "/fpga_ddr/DRAM_ADDR6")
	(net 19 "/fpga_ddr/DRAM_ADDR1")
	(net 20 "/fpga_ddr/DRAM_ADDR0")
	(net 21 "/fpga_ddr/DRAM_CSB")
	(net 22 "/fpga_ddr/DRAM_CASB")
	(net 23 "/fpga_ddr/DRAM_DATA7")
	(net 24 "/fpga_ddr/DRAM_DATA5")
	(net 25 "Net-(U5-FB)")
	(net 26 "/fpga_ddr/DRAM_DATA1")
	(net 27 "/fpga_ddr/DRAM_ADDR13")
	(net 28 "/fpga_ddr/DRAM_ADDR9")
	(net 29 "/fpga_ddr/DRAM_ADDR5")
	(net 30 "/fpga_ddr/DRAM_ADDR2")
	(net 31 "/fpga_ddr/DRAM_BA0")
	(net 32 "/fpga_ddr/DRAM_RASB")
	(net 33 "/fpga_ddr/DRAM_WEB")
	(net 34 "/fpga_ddr/DRAM_DATA6")
	(net 35 "/fpga_ddr/DRAM_DATA4")
	(net 36 "/fpga_ddr/DRAM_DATA13")
	(net 37 "/fpga_ddr/DRAM_DATA12")
	(net 38 "/fpga_ddr/DRAM_ADDR12")
	(net 39 "/fpga_ddr/DRAM_ADDR11")
	(net 40 "/fpga_ddr/DRAM_ADDR8")
	(net 41 "/fpga_ddr/DRAM_ADDR7")
	(net 42 "/fpga_ddr/DRAM_BA1")
	(net 43 "/fpga_ddr/DRAM_CKE")
	(net 44 "/fpga_ddr/DRAM_ODT")
	(net 45 "/fpga_ddr/DRAM_DATA3")
	(net 46 "/fpga_ddr/DRAM_DATA2")
	(net 47 "Net-(U24-FB)")
	(net 48 "/fpga_ddr/DRAM_DATA14")
	(net 49 "/fpga_ddr/DRAM_DATA10")
	(net 50 "/fpga_ddr/DRAM_DATA8")
	(net 51 "/fpga_ddr/DRAM_ADDR4")
	(net 52 "/fpga_ddr/DRAM_ADDR3")
	(net 53 "/fpga_ddr/DRAM_BA2")
	(net 54 "/fpga_ddr/DRAM_RST")
	(net 55 "/fpga_ddr/DRAM_DATA0")
	(net 56 "/fpga_ddr/DRAM_DATA15")
	(net 57 "/fpga_ddr/DRAM_DATA11")
	(net 58 "/fpga_ddr/DRAM_DATA9")
	(net 59 "Net-(U26-BS)")
	(net 60 "+1V2_FPGA")
	(net 61 "Net-(U26-FB)")
	(net 62 "EPDC_SE_CLK")
	(net 63 "FL_PWM1")
	(net 64 "FL_PWM2")
	(net 65 "FPGA_TDI")
	(net 66 "FPGA_TCK")
	(net 67 "FPGA_TMS")
	(net 68 "FPGA_TDO")
	(net 69 "/epd_power/EN_VGL")
	(net 70 "+5V")
	(net 71 "/dp_in/TX1N")
	(net 72 "/dp_in/TX1NC")
	(net 73 "/dp_in/TX1P")
	(net 74 "Net-(D1-A)")
	(net 75 "Net-(D1-K)")
	(net 76 "Net-(D4-K)")
	(net 77 "Net-(D8-A)")
	(net 78 "Net-(D15-A)")
	(net 79 "/dp_in/TX1PC")
	(net 80 "Net-(D20-A)")
	(net 81 "/dp_in/RX1N")
	(net 82 "KEY2")
	(net 83 "/dp_in/RX1NC")
	(net 84 "EPDC_D7P")
	(net 85 "EPDC_D3N")
	(net 86 "EPDC_D10N")
	(net 87 "EPDC_D0P")
	(net 88 "EPD_PWR_EN")
	(net 89 "VBUS_MEA")
	(net 90 "EPDC_D7N")
	(net 91 "unconnected-(J4-CEC-Pad14)")
	(net 92 "EPDC_D11P")
	(net 93 "EPDC_D9N")
	(net 94 "EPDC_D2P")
	(net 95 "EPDC_D5P")
	(net 96 "EPDC_D10P")
	(net 97 "-VGL")
	(net 98 "+VGH")
	(net 99 "Net-(U2-SW)")
	(net 100 "Net-(U2-BS)")
	(net 101 "EPDC_D0N")
	(net 102 "EPDC_D9P")
	(net 103 "-VN")
	(net 104 "Net-(U2-FB)")
	(net 105 "EPDC_D8P")
	(net 106 "Net-(U9-BS)")
	(net 107 "Net-(U9-FB)")
	(net 108 "Net-(U23-FB)")
	(net 109 "Net-(U11-+)")
	(net 110 "EPDC_D4P")
	(net 111 "Net-(D2-A)")
	(net 112 "EPDC_D11N")
	(net 113 "EPDC_D1P")
	(net 114 "EPDC_D6N")
	(net 115 "/dp_in/RX1P")
	(net 116 "EPDC_CLKN")
	(net 117 "/dp_in/RX1PC")
	(net 118 "EPDC_D2N")
	(net 119 "Net-(U15-XTALP)")
	(net 120 "/dp_in/TX2N")
	(net 121 "unconnected-(U21-WARNING-Pad8)")
	(net 122 "unconnected-(U21-PV-Pad10)")
	(net 123 "unconnected-(U21-TC-Pad13)")
	(net 124 "unconnected-(J4-UTILITY-Pad17)")
	(net 125 "Net-(Q1-G)")
	(net 126 "Net-(Q2-B)")
	(net 127 "Net-(U4-SET)")
	(net 128 "EPDC_CLKP")
	(net 129 "EPDC_D1N")
	(net 130 "Net-(U6-SET)")
	(net 131 "EPDC_D8N")
	(net 132 "EPDC_D3P")
	(net 133 "EPDC_D6P")
	(net 134 "EPDC_D4N")
	(net 135 "EPDC_D5N")
	(net 136 "MCU_SWDIO")
	(net 137 "unconnected-(U22-TC-Pad13)")
	(net 138 "SDIO_CMD")
	(net 139 "SDIO_CLK")
	(net 140 "I2C1_SDA")
	(net 141 "I2C1_SCL")
	(net 142 "unconnected-(U22-PV-Pad10)")
	(net 143 "KEY3")
	(net 144 "/fpga_io/LED")
	(net 145 "VGH_MEA")
	(net 146 "Net-(X1-OUT)")
	(net 147 "/dp_in/TX2NC")
	(net 148 "/dp_in/TX2P")
	(net 149 "/dp_in/TX2PC")
	(net 150 "/dp_in/RX2N")
	(net 151 "/dp_in/RX2NC")
	(net 152 "Net-(Q6-G)")
	(net 153 "Net-(Q6-S)")
	(net 154 "Net-(Q7-G)")
	(net 155 "Net-(Q8-G)")
	(net 156 "VCOM_MEA")
	(net 157 "Net-(Q8-D)")
	(net 158 "VCOM_EN")
	(net 159 "VCOM_MEA_EN")
	(net 160 "/dp_in/RX2P")
	(net 161 "/dp_in/RX2PC")
	(net 162 "/dp_in/SBU1")
	(net 163 "/dp_in/DPAUXP")
	(net 164 "/dp_in/SBU2")
	(net 165 "/dp_in/DPAUXN")
	(net 166 "Net-(C117-Pad1)")
	(net 167 "Net-(C118-Pad1)")
	(net 168 "/dp_in/CC1")
	(net 169 "USB_DP")
	(net 170 "USB_DN")
	(net 171 "/dp_in/CC2")
	(net 172 "Net-(U15-XTALN)")
	(net 173 "/tmds_in/TMDS_D1N")
	(net 174 "DP_PDN")
	(net 175 "Net-(U19-TESTMODE)")
	(net 176 "DP_HPD")
	(net 177 "TYPEC_ORI")
	(net 178 "TCPC_INT")
	(net 179 "/dp_in/DP1N")
	(net 180 "/dp_in/DP1P")
	(net 181 "/dp_in/DP0N")
	(net 182 "/dp_in/DP0P")
	(net 183 "/tmds_in/TMDS_D1P")
	(net 184 "unconnected-(U19-DEV_CFG-Pad12)")
	(net 185 "unconnected-(U19-NC-Pad15)")
	(net 186 "unconnected-(U19-NC-Pad16)")
	(net 187 "unconnected-(U19-CFG1-Pad21)")
	(net 188 "unconnected-(U19-CFG2-Pad22)")
	(net 189 "unconnected-(U19-CFG3-Pad23)")
	(net 190 "VGL_MEA")
	(net 191 "unconnected-(U19-CFG4-Pad27)")
	(net 192 "unconnected-(U19-PWMO-Pad28)")
	(net 193 "unconnected-(U19-DDC_SCL-Pad29)")
	(net 194 "unconnected-(U19-DDC_SDA-Pad30)")
	(net 195 "unconnected-(U19-LVSDE_N-Pad31)")
	(net 196 "unconnected-(U19-LVSDE_P-Pad32)")
	(net 197 "LVDS_BKLTEN")
	(net 198 "LVDS_EVEN_CP")
	(net 199 "LVDS_EVEN_CN")
	(net 200 "LVDS_EVEN_BP")
	(net 201 "LVDS_EVEN_BN")
	(net 202 "LVDS_EVEN_AP")
	(net 203 "LVDS_EVEN_AN")
	(net 204 "unconnected-(U19-LVSDO_P-Pad43)")
	(net 205 "unconnected-(U19-LVSDO_N-Pad44)")
	(net 206 "LVDS_ODD_CP")
	(net 207 "LVDS_ODD_CN")
	(net 208 "LVDS_ODD_BP")
	(net 209 "LVDS_ODD_BN")
	(net 210 "LVDS_ODD_AP")
	(net 211 "LVDS_ODD_AN")
	(net 212 "unconnected-(U19-NC-Pad55)")
	(net 213 "/tmds_in/TMDS_D2N")
	(net 214 "/tmds_in/TMDS_D2P")
	(net 215 "/tmds_in/TMDS_CKN")
	(net 216 "/tmds_in/TMDS_CKP")
	(net 217 "/tmds_in/TMDS_D0N")
	(net 218 "/tmds_in/TMDS_D0P")
	(net 219 "/tmds_in/HDMI_SCL")
	(net 220 "/tmds_in/HDMI_SDA")
	(net 221 "EPD_POS_EN")
	(net 222 "/tmds_in/HDMI_HPD")
	(net 223 "DPI_DE")
	(net 224 "DPI_HS")
	(net 225 "DPI_VS")
	(net 226 "DPI_PCLK")
	(net 227 "DPI_G3")
	(net 228 "DPI_G2")
	(net 229 "DPI_G7")
	(net 230 "DPI_G6")
	(net 231 "DPI_G5")
	(net 232 "DPI_G4")
	(net 233 "DPI_R7")
	(net 234 "DPI_R6")
	(net 235 "DPI_R5")
	(net 236 "DPI_R4")
	(net 237 "DPI_R3")
	(net 238 "DPI_R2")
	(net 239 "DPI_B7")
	(net 240 "DPI_B6")
	(net 241 "DPI_B5")
	(net 242 "DPI_B4")
	(net 243 "DPI_B3")
	(net 244 "DPI_B2")
	(net 245 "unconnected-(U15-AP-Pad48)")
	(net 246 "unconnected-(U15-SCLK{slash}INT2-Pad49)")
	(net 247 "unconnected-(U15-LRCLK-Pad50)")
	(net 248 "unconnected-(U15-MCLK{slash}INT2-Pad51)")
	(net 249 "DEC_RST")
	(net 250 "unconnected-(U15-CEC-Pad61)")
	(net 251 "/tmds_in/ADV_CK")
	(net 252 "/tmds_in/ADV_DE")
	(net 253 "/tmds_in/ADV_HS")
	(net 254 "/tmds_in/ADV_VS")
	(net 255 "/tmds_in/ADV_P8")
	(net 256 "/tmds_in/ADV_P11")
	(net 257 "/tmds_in/ADV_P10")
	(net 258 "/tmds_in/ADV_P9")
	(net 259 "/tmds_in/ADV_P13")
	(net 260 "/tmds_in/ADV_P14")
	(net 261 "/tmds_in/ADV_P15")
	(net 262 "/tmds_in/ADV_P12")
	(net 263 "/tmds_in/ADV_P21")
	(net 264 "/tmds_in/ADV_P23")
	(net 265 "/tmds_in/ADV_P22")
	(net 266 "/tmds_in/ADV_P20")
	(net 267 "/tmds_in/ADV_P17")
	(net 268 "/tmds_in/ADV_P19")
	(net 269 "/tmds_in/ADV_P18")
	(net 270 "/tmds_in/ADV_P16")
	(net 271 "/tmds_in/ADV_P6")
	(net 272 "/tmds_in/ADV_P7")
	(net 273 "/tmds_in/ADV_P4")
	(net 274 "/tmds_in/ADV_P5")
	(net 275 "/tmds_in/ADV_P0")
	(net 276 "/tmds_in/ADV_P1")
	(net 277 "/tmds_in/ADV_P2")
	(net 278 "/tmds_in/ADV_P3")
	(net 279 "Net-(U20-BS)")
	(net 280 "Net-(U20-SW)")
	(net 281 "Net-(U20-FB)")
	(net 282 "unconnected-(U19-VDD18REG-Pad19)")
	(net 283 "unconnected-(U22-WARNING-Pad8)")
	(net 284 "-VCOM")
	(net 285 "+1V2_DCDC")
	(net 286 "+VP")
	(net 287 "+5V2_FL")
	(net 288 "unconnected-(U1C-IO_L29N_GCLK2_2-PadN8)")
	(net 289 "SDIO_DAT3")
	(net 290 "SDIO_DAT0")
	(net 291 "SDIO_DAT2")
	(net 292 "SDIO_DAT1")
	(net 293 "unconnected-(U22-CRITICAL-Pad9)")
	(net 294 "VCOM_DAC")
	(net 295 "unconnected-(U27-WARNING-Pad8)")
	(net 296 "unconnected-(U27-CRITICAL-Pad9)")
	(net 297 "unconnected-(U27-TC-Pad13)")
	(net 298 "unconnected-(U27-PV-Pad10)")
	(net 299 "+3V3_DCDC")
	(net 300 "+1V35_DCDC")
	(net 301 "+3V3")
	(net 302 "+5V_ES")
	(net 303 "+5V_EG")
	(net 304 "+1V35")
	(net 305 "+1V8_VID")
	(net 306 "+3V3_VID")
	(net 307 "+1V8_DCDC")
	(net 308 "/power/EVDD")
	(net 309 "Net-(U13-FB)")
	(net 310 "Net-(U13-VIN)")
	(net 311 "Net-(U13-SW2)")
	(net 312 "Net-(U13-BST2)")
	(net 313 "Net-(U13-BST1)")
	(net 314 "Net-(U13-SW1)")
	(net 315 "GND")
	(net 316 "QSPI_SCLK")
	(net 317 "LVDS_PVCCEN")
	(net 318 "unconnected-(U15-INT1-Pad55)")
	(net 319 "Net-(J1-D+-PadA6)")
	(net 320 "Net-(J1-D--PadA7)")
	(net 321 "unconnected-(RN7-R1.2-Pad8)")
	(net 322 "unconnected-(RN7-R1.1-Pad1)")
	(net 323 "Net-(D19-A)")
	(net 324 "+VBUS")
	(net 325 "+5V_HDMI")
	(net 326 "FL_EN")
	(net 327 "MCU_SWCLK")
	(net 328 "unconnected-(J7-Pad9)")
	(net 329 "VGH_DAC")
	(net 330 "/epd_power/EN_VN")
	(net 331 "FPGA_PROG")
	(net 332 "FPGA_SUSP")
	(net 333 "FPGA_DONE")
	(net 334 "Net-(U1D-IO_L1P_3)")
	(net 335 "/mcu/G_LED")
	(net 336 "/mcu/R_LED")
	(net 337 "VP_MEA")
	(net 338 "Net-(U12-ZQ)")
	(net 339 "GCLK")
	(net 340 "VN_MEA")
	(net 341 "unconnected-(RN8-R1.2-Pad8)")
	(net 342 "unconnected-(RN8-R2.2-Pad7)")
	(net 343 "unconnected-(RN11-R1.2-Pad8)")
	(net 344 "unconnected-(RN11-R2.2-Pad7)")
	(net 345 "unconnected-(RN13-R2.2-Pad7)")
	(net 346 "unconnected-(RN13-R1.2-Pad8)")
	(net 347 "KEY1")
	(net 348 "unconnected-(U1C-IO_L16N_VREF_2-PadM10)")
	(net 349 "unconnected-(U1C-IO_L31N_GCLK30_D15_2-PadM7)")
	(net 350 "FPGA_MOSI")
	(net 351 "unconnected-(U1C-IO_L31P_GCLK31_D14_2-PadP7)")
	(net 352 "unconnected-(U1B-IO_L1N_A24_VREF_1-PadE12)")
	(net 353 "unconnected-(U1B-IO_L50N_M1UDQSN_1-PadT15)")
	(net 354 "EPD_THROT")
	(net 355 "unconnected-(U1B-IO_L49P_M1DQ10_1-PadR15)")
	(net 356 "FPGA_CS")
	(net 357 "unconnected-(U1B-IO_L40P_GCLK11_M1A5_1-PadJ11)")
	(net 358 "LVDS_ODD_CKN")
	(net 359 "unconnected-(U19-LVSCKE_N-Pad35)")
	(net 360 "LVDS_ODD_CKP")
	(net 361 "unconnected-(U1D-IO_L2N_3-PadN4)")
	(net 362 "unconnected-(U19-LVSCKE_P-Pad34)")
	(net 363 "/fpga_config/FPGA_INIT")
	(net 364 "unconnected-(U1B-IO_L32P_A17_M1A8_1-PadF13)")
	(net 365 "/mcu/OSC_IN")
	(net 366 "Net-(C10-Pad1)")
	(net 367 "FPGA_MISO")
	(net 368 "/mcu/OSC32_IN")
	(net 369 "/mcu/OSC32_OUT")
	(net 370 "unconnected-(U1B-IO_L30N_A20_M1A11_1-PadG11)")
	(net 371 "Net-(U3-NRST)")
	(net 372 "unconnected-(U1D-IO_L2P_3-PadM5)")
	(net 373 "unconnected-(U1D-IO_L83P_3-PadB3)")
	(net 374 "+3V3A")
	(net 375 "unconnected-(U1B-IO_L30P_A21_M1RESET_1-PadF12)")
	(net 376 "/fpga_ddr/DRAM_UDQSN")
	(net 377 "unconnected-(U1C-IO_L12N_D2_MISO3_2-PadP12)")
	(net 378 "unconnected-(U1C-IO_L12P_D1_MISO2_2-PadN12)")
	(net 379 "/mcu/OSC_OUT")
	(net 380 "unconnected-(U1C-IO_L13N_D10_2-PadP11)")
	(net 381 "FPGA_SCLK")
	(net 382 "unconnected-(U1C-IO_L49P_D3_2-PadN5)")
	(net 383 "Net-(C145-Pad2)")
	(net 384 "unconnected-(U1B-IO_L38N_A4_M1CLKN_1-PadH11)")
	(net 385 "/fpga_ddr/DRAM_UDQSP")
	(net 386 "unconnected-(U1C-IO_L65N_CSO_B_2-PadT3)")
	(net 387 "unconnected-(U1C-IO_L64P_D8_2-PadM6)")
	(net 388 "unconnected-(U1C-IO_L62N_D6_2-PadL7)")
	(net 389 "/fpga_ddr/DRAM_LDQSN")
	(net 390 "/fpga_ddr/DRAM_LDQSP")
	(net 391 "unconnected-(U1C-IO_L62P_D5_2-PadL8)")
	(net 392 "unconnected-(U1C-IO_L64N_D9_2-PadN6)")
	(net 393 "unconnected-(U1E-CMPCS_B_2-PadL11)")
	(net 394 "/fpga_ddr/DRAM_UDM")
	(net 395 "unconnected-(U1C-IO_L14N_D12_2-PadP9)")
	(net 396 "unconnected-(U1C-IO_L49N_D4_2-PadP5)")
	(net 397 "/fpga_ddr/DRAM_LDM")
	(net 398 "unconnected-(U1C-IO_L14P_D11_2-PadN9)")
	(net 399 "unconnected-(U3-PC8-Pad65)")
	(net 400 "FMC_D0")
	(net 401 "unconnected-(U3-PB11-Pad47)")
	(net 402 "FMC_D1")
	(net 403 "unconnected-(U3-PC6-Pad63)")
	(net 404 "unconnected-(U3-PA8-Pad67)")
	(net 405 "FMC_A16")
	(net 406 "FMC_D6")
	(net 407 "QSPI_SS")
	(net 408 "FMC_D5")
	(net 409 "QSPI_SD3")
	(net 410 "FMC_NOE")
	(net 411 "unconnected-(U3-PC13-Pad7)")
	(net 412 "QSPI_SD1")
	(net 413 "unconnected-(U3-PC0-Pad15)")
	(net 414 "FMC_NE1")
	(net 415 "FMC_D7")
	(net 416 "FMC_D3")
	(net 417 "FMC_NWE")
	(net 418 "FMC_D2")
	(net 419 "QSPI_SD2")
	(net 420 "QSPI_SD0")
	(net 421 "FMC_D4")
	(net 422 "unconnected-(U12-A15{slash}NC-PadM7)")
	(net 423 "unconnected-(U1A-IO_L2P_0-PadB5)")
	(net 424 "unconnected-(U1A-IO_L4P_0-PadB6)")
	(net 425 "unconnected-(U1A-IO_L5P_0-PadF7)")
	(net 426 "unconnected-(U1A-IO_L1P_HSWAPEN_0-PadC4)")
	(net 427 "unconnected-(U1A-IO_L5N_0-PadE6)")
	(net 428 "unconnected-(U1A-IO_L7N_0-PadC6)")
	(net 429 "unconnected-(U1A-IO_L1N_VREF_0-PadA4)")
	(net 430 "unconnected-(U1A-IO_L7P_0-PadD6)")
	(net 431 "unconnected-(U1A-IO_L4N_0-PadA6)")
	(net 432 "unconnected-(U1A-IO_L2N_0-PadA5)")
	(net 433 "unconnected-(U1A-IO_L3N_0-PadC5)")
	(net 434 "unconnected-(U1A-IO_L3P_0-PadD5)")
	(net 435 "unconnected-(U1A-IO_L40N_0-PadD9)")
	(net 436 "unconnected-(U1A-IO_L40P_0-PadF9)")
	(net 437 "unconnected-(U1B-IO_L32N_A16_M1A9_1-PadF14)")
	(net 438 "unconnected-(U1B-IO_L1P_A25_1-PadE13)")
	(net 439 "+5V_DCDC")
	(net 440 "unconnected-(J6-Pin_50-Pad50)")
	(net 441 "unconnected-(J6-Pin_46-Pad46)")
	(net 442 "unconnected-(J6-Pin_2-Pad2)")
	(net 443 "unconnected-(J6-Pin_4-Pad4)")
	(net 444 "unconnected-(J6-Pin_48-Pad48)")
	(net 445 "USER_PB9")
	(net 446 "USER_PD10")
	(net 447 "USER_PD8")
	(net 448 "USER_PD13")
	(net 449 "USER_PB8")
	(net 450 "USER_PD9")
	(net 451 "Net-(U15-HPA_A{slash}INT2)")
	(net 452 "/epd_power/+5V_VSH")
	(net 453 "/epd_power/+5V_VGH")
	(net 454 "Net-(U3-PE11)")
	(net 455 "HPD_EN")
	(net 456 "Net-(U10-SET)")
	(net 457 "Net-(U10-VOUT)")
	(net 458 "Net-(D3-K)")
	(net 459 "Net-(D17-K)")
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.925 102.49 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.29 1.525 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U5-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Xunpu_FPC-05F-16PH20_1x16-1MP_P0.50mm_Horizontal"
		(layer "F.Cu")
		(at 69.7 96.5 -90)
		(descr "Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
		(tags "connector Hirose FH12 horizontal")
		(property "Reference" "J3"
			(at -7.1 3.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FPC-05F-16PH20"
			(at 0 5.6 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:Xunpu_FPC-05F-16PH20_1x16-1MP_P0.50mm_Horizontal"
			(at 0 -0.05 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -0.05 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 -0.05 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2856801"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "EPDC_CLKN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "EPDC_CLKP")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "EPDC_D11N")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -1.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "EPDC_D11P")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -0.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "EPDC_D10N")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "EPDC_D10P")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 1.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "EPDC_D9N")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "EPDC_D9P")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 2.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 2.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "EPDC_D8N")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 3.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "EPDC_D8P")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 3.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -5.44 0.75 270)
			(size 1.8 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 5.44 0.75 270)
			(size 2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FPC-SMD_16P-P0.50_FPC-05F-16PH20.step"
			(offset
				(xyz 0 1.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 112.18 53.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C89"
			(at 0.02 4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 383 "Net-(C145-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.69 50.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R97"
			(at -1.99 -0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "VGH_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 109 41.6 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q8"
			(at 0 -5.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AO3401A"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C347476"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "Net-(Q8-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "VCOM_MEA")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 157 "Net-(Q8-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 101.5375 53.55)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 2.6625 0.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AO3401A"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C347476"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(D1-A)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91.6 65.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C186"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 112.2 49.4)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1K/1%"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "EPD_PWR_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 454 "Net-(U3-PE11)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 140.9 77.2 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C91"
			(at 0.2 -2.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "VBUS_MEA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 119.05 32.2)
		(property "Reference" "H8"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -0.09 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR4020S"
		(layer "F.Cu")
		(at 131.7 68.95 90)
		(descr "Inductor, Changjiang, FNR4020S, 4.0x4.0x2.0mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L15"
			(at 0 -3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN4020H2R2MT"
			(at 0 3 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR4020S"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98361"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.1 3.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 311 "Net-(U13-SW2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.1 3.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 314 "Net-(U13-SW1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR4020S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 132.7 71.8 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C100"
			(at 2.3 -0.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 312 "Net-(U13-BST2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 311 "Net-(U13-SW2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-6"
		(layer "F.Cu")
		(at 104.7625 103)
		(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at -0.0625 3.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SY8113C"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6338414"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT*23*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U2-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "Net-(U2-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 80.05 47.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at -2.05 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U9-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 84.55 49.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 5.75 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 90.755 57.11)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R61"
			(at -0.155 1.49 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 124.62 94.25 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C136"
			(at 0.250001 -0.92 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 105 83)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L3"
			(at 0 -2.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(U28-SW)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 285 "+1V2_DCDC")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 134.1 46.65 90)
		(property "Reference" "H5"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.01 -0.02 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.2 57.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R94"
			(at 8.8 1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "/epd_power/EN_VGL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 100.6 93.1125 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R56"
			(at 2.8875 0.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 300 "+1V35_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 119.525 88.9 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C152"
			(at -4.675 0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 93.25 36.8 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D15"
			(at 2.85 -0.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.45 -0.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(D15-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.7 64.9 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C95"
			(at -0.5 3.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14442"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 309 "Net-(U13-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 138.72 87.4 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN10"
			(at 0.4 1.88 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 266 "/tmds_in/ADV_P20")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 263 "/tmds_in/ADV_P21")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 265 "/tmds_in/ADV_P22")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 264 "/tmds_in/ADV_P23")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 233 "DPI_R7")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 234 "DPI_R6")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 235 "DPI_R5")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 236 "DPI_R4")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 121.325 90.4875)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C142"
			(at 0.875 -0.8875 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
		(layer "F.Cu")
		(at 104.325 92.4625 180)
		(descr "Texas RGV0016A VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/ina3221.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U27"
			(at -3.875 -0.3375 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "INA3221"
			(at 0 3.33 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina3221.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Triple-Channel High-Side Shunt and Bus Voltage Monitor with I2C and SMBUS Compatible Interface, QFN-16"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C181255"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*RGV0016A*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.525 -0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.525 0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.525 -0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.525 0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.8625 -0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "IN-3")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.8625 -0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "IN+3")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.8625 0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -1.8625 0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -0.975 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -0.325 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 0.325 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 0.975 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 295 "unconnected-(U27-WARNING-Pad8)")
			(pinfunction "WARNING")
			(pintype "open_collector+no_connect")
		)
		(pad "9" smd roundrect
			(at 1.8625 0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 296 "unconnected-(U27-CRITICAL-Pad9)")
			(pinfunction "CRITICAL")
			(pintype "open_collector+no_connect")
		)
		(pad "10" smd roundrect
			(at 1.8625 0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 298 "unconnected-(U27-PV-Pad10)")
			(pinfunction "PV")
			(pintype "open_collector+no_connect")
		)
		(pad "11" smd roundrect
			(at 1.8625 -0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pinfunction "IN-1")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 1.8625 -0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 300 "+1V35_DCDC")
			(pinfunction "IN+1")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 0.975 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 297 "unconnected-(U27-TC-Pad13)")
			(pinfunction "TC")
			(pintype "open_collector+no_connect")
		)
		(pad "14" smd roundrect
			(at 0.325 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pinfunction "IN-2")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -0.325 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 285 "+1V2_DCDC")
			(pinfunction "IN+2")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at -0.975 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "VPU")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 2.1 2.1)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "EP")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.1 37.2)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R87"
			(at 1.9 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 337 "VP_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 105.9 105.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(at 68.5 106.5)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H3"
			(at 0 -2.9 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 2.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "DNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 114.925 104.6 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 0.925 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25768"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U5-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 133.47 87.4 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C137"
			(at 2.6 -0.87 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 126 104.6 180)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U10"
			(at 0 -2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MT9700"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C89855"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 457 "Net-(U10-VOUT)")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 456 "Net-(U10-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 455 "HPD_EN")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:QFN15_3X4_JW3651"
		(layer "F.Cu")
		(at 135.9 68.7 180)
		(property "Reference" "U13"
			(at 0.67351 3.412998 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JW3651QFNE"
			(at -5.29356 -3.699002 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "footprints:QFN15_3X4_JW3651"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5444670"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(pad "1" smd rect
			(at -1.5 -1.25 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "CSP")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "2" smd custom
			(at -1.9 -0.85001)
			(size 0.000001 0.000001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 310 "Net-(U13-VIN)")
			(pinfunction "VIN")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.000001)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.2) (xy -0.65 -0.2) (xy -0.82 -0.37) (xy -1.62 -0.37) (xy -1.62 -0.17) (xy -0.95 -0.17)
						(xy -0.78 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd circle
			(at -1.09 -0.66501 180)
			(size 0.0254 0.0254)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 310 "Net-(U13-VIN)")
			(pinfunction "VIN")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 90)
		)
		(pad "3" smd rect
			(at -1.09 0.25 180)
			(size 1.62 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "PGND")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd custom
			(at -1.9 1.34999)
			(size 0.000001 0.000001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 439 "+5V_DCDC")
			(pinfunction "VO")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.000001)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 0.19999) (xy -0.65 0.19999) (xy -0.82 0.36999) (xy -1.62 0.37) (xy -1.62 0.16999)
						(xy -0.95 0.16999) (xy -0.78 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "4" smd circle
			(at -1.09 1.165 180)
			(size 0.0254 0.0254)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 439 "+5V_DCDC")
			(pinfunction "VO")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 90)
		)
		(pad "5" smd roundrect
			(at -0.75 2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 309 "Net-(U13-FB)")
			(pinfunction "FB")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd roundrect
			(at -0.25 2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 315 "GND")
			(pinfunction "OLIM")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd roundrect
			(at 0.25 2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 308 "/power/EVDD")
			(pinfunction "EN")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd roundrect
			(at 0.75 2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 313 "Net-(U13-BST1)")
			(pinfunction "BST1")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd custom
			(at 0.25 0.51)
			(size 0.000001 0.000001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 314 "Net-(U13-SW1)")
			(pinfunction "SW1")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.000001)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.19999) (xy -0.73 -0.2) (xy -0.87 -0.34) (xy -1.65 -0.34) (xy -1.65 -0.14) (xy -1.1 -0.14)
						(xy -0.96 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd circle
			(at 1.075 0.68 180)
			(size 0.0254 0.0254)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 314 "Net-(U13-SW1)")
			(pinfunction "SW1")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 90)
		)
		(pad "10" smd custom
			(at 0.25 -0.01)
			(size 0.000001 0.000001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 311 "Net-(U13-SW2)")
			(pinfunction "SW2")
			(pintype "input")
			(solder_mask_margin 0.05)
			(solder_paste_margin 0.000001)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 0.2) (xy -0.73 0.2) (xy -0.87 0.34) (xy -1.65 0.34) (xy -1.65 0.14) (xy -1.1 0.14001)
						(xy -0.96 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "10" smd circle
			(at 1.075 -0.18 180)
			(size 0.0254 0.0254)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 311 "Net-(U13-SW2)")
			(pinfunction "SW2")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 90)
		)
		(pad "11" smd rect
			(at 1.5 -1.25 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 312 "Net-(U13-BST2)")
			(pinfunction "BST2")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "12" smd roundrect
			(at 0.75 -2.00001 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 315 "GND")
			(pinfunction "TEST")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "13" smd roundrect
			(at 0.25 -2.00001 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 308 "/power/EVDD")
			(pinfunction "VCC")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "14" smd roundrect
			(at -0.25 -2.00001 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(pad "15" smd roundrect
			(at -0.75 -2.00001 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15)
			(net 308 "/power/EVDD")
			(pinfunction "CSN")
			(pintype "input")
			(solder_mask_margin 0.05)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_3x4mm_P0.4mm_EP1.65x2.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 138.9 106 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at -0.05 -1.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 220 "/tmds_in/HDMI_SDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 325 "+5V_HDMI")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-64-1EP_10x10mm_P0.5mm_EP5x5mm"
		(layer "F.Cu")
		(at 133.12 95.4 180)
		(descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/adv7611.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U15"
			(at 6.4 -4.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ADV7611"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_QFP:LQFP-64-1EP_10x10mm_P0.5mm_EP5x5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adv7611.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C146553"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LQFP*1EP*10x10mm*P0.5mm*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -2 -2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -2 -1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -2 0 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -2 1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -2 2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1 -2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1 -1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1 0 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1 1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1 2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 -2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 -1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1 -2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1 -1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1 0 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1 1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1 2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 2 -2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 2 -1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 2 0 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 2 1 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 2 2 180)
			(size 0.81 0.81)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -5.675 -3.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 451 "Net-(U15-HPA_A{slash}INT2)")
			(pinfunction "HPA_A/INT2")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -5.675 -3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "CVDD")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -5.675 -2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "/tmds_in/TMDS_CKN")
			(pinfunction "RXA_C-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.675 -2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 216 "/tmds_in/TMDS_CKP")
			(pinfunction "RXA_C+")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.675 -1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "TVDD")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -5.675 -1.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 217 "/tmds_in/TMDS_D0N")
			(pinfunction "RXA_0-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.675 -0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 218 "/tmds_in/TMDS_D0P")
			(pinfunction "RXA_0+")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.675 -0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "TVDD")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -5.675 0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 173 "/tmds_in/TMDS_D1N")
			(pinfunction "RXA_1-")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.675 0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 183 "/tmds_in/TMDS_D1P")
			(pinfunction "RXA_1+")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.675 1.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "TVDD")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -5.675 1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 213 "/tmds_in/TMDS_D2N")
			(pinfunction "RXA_2-")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -5.675 2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "/tmds_in/TMDS_D2P")
			(pinfunction "RXA_2+")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at -5.675 2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "CVDD")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at -5.675 3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 264 "/tmds_in/ADV_P23")
			(pinfunction "P23")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at -5.675 3.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 265 "/tmds_in/ADV_P22")
			(pinfunction "P22")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -3.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 263 "/tmds_in/ADV_P21")
			(pinfunction "P21")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at -3.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 266 "/tmds_in/ADV_P20")
			(pinfunction "P20")
			(pintype "output")
		)
		(pad "19" smd roundrect
			(at -2.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 268 "/tmds_in/ADV_P19")
			(pinfunction "P19")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at -2.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 269 "/tmds_in/ADV_P18")
			(pinfunction "P18")
			(pintype "output")
		)
		(pad "21" smd roundrect
			(at -1.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 267 "/tmds_in/ADV_P17")
			(pinfunction "P17")
			(pintype "output")
		)
		(pad "22" smd roundrect
			(at -1.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 270 "/tmds_in/ADV_P16")
			(pinfunction "P16")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at -0.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "DVDDIO")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at -0.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "25" smd roundrect
			(at 0.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 251 "/tmds_in/ADV_CK")
			(pinfunction "LLC")
			(pintype "output")
		)
		(pad "26" smd roundrect
			(at 0.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 261 "/tmds_in/ADV_P15")
			(pinfunction "P15")
			(pintype "output")
		)
		(pad "27" smd roundrect
			(at 1.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 260 "/tmds_in/ADV_P14")
			(pinfunction "P14")
			(pintype "output")
		)
		(pad "28" smd roundrect
			(at 1.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 259 "/tmds_in/ADV_P13")
			(pinfunction "P13")
			(pintype "output")
		)
		(pad "29" smd roundrect
			(at 2.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 262 "/tmds_in/ADV_P12")
			(pinfunction "P12")
			(pintype "output")
		)
		(pad "30" smd roundrect
			(at 2.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 256 "/tmds_in/ADV_P11")
			(pinfunction "P11")
			(pintype "output")
		)
		(pad "31" smd roundrect
			(at 3.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 257 "/tmds_in/ADV_P10")
			(pinfunction "P10")
			(pintype "output")
		)
		(pad "32" smd roundrect
			(at 3.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 258 "/tmds_in/ADV_P9")
			(pinfunction "P9")
			(pintype "output")
		)
		(pad "33" smd roundrect
			(at 5.675 3.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 255 "/tmds_in/ADV_P8")
			(pinfunction "P8")
			(pintype "output")
		)
		(pad "34" smd roundrect
			(at 5.675 3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "DVDDIO")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at 5.675 2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 272 "/tmds_in/ADV_P7")
			(pinfunction "P7")
			(pintype "output")
		)
		(pad "36" smd roundrect
			(at 5.675 2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 271 "/tmds_in/ADV_P6")
			(pinfunction "P6")
			(pintype "output")
		)
		(pad "37" smd roundrect
			(at 5.675 1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 274 "/tmds_in/ADV_P5")
			(pinfunction "P5")
			(pintype "output")
		)
		(pad "38" smd roundrect
			(at 5.675 1.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 273 "/tmds_in/ADV_P4")
			(pinfunction "P4")
			(pintype "output")
		)
		(pad "39" smd roundrect
			(at 5.675 0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 278 "/tmds_in/ADV_P3")
			(pinfunction "P3")
			(pintype "output")
		)
		(pad "40" smd roundrect
			(at 5.675 0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "41" smd roundrect
			(at 5.675 -0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 277 "/tmds_in/ADV_P2")
			(pinfunction "P2")
			(pintype "output")
		)
		(pad "42" smd roundrect
			(at 5.675 -0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 276 "/tmds_in/ADV_P1")
			(pinfunction "P1")
			(pintype "output")
		)
		(pad "43" smd roundrect
			(at 5.675 -1.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 275 "/tmds_in/ADV_P0")
			(pinfunction "P0")
			(pintype "output")
		)
		(pad "44" smd roundrect
			(at 5.675 -1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "DVDDIO")
			(pintype "power_in")
		)
		(pad "45" smd roundrect
			(at 5.675 -2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 252 "/tmds_in/ADV_DE")
			(pinfunction "DE")
			(pintype "output")
		)
		(pad "46" smd roundrect
			(at 5.675 -2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 253 "/tmds_in/ADV_HS")
			(pinfunction "HS")
			(pintype "output")
		)
		(pad "47" smd roundrect
			(at 5.675 -3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 254 "/tmds_in/ADV_VS")
			(pinfunction "VS/FIELD/ALSB")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 5.675 -3.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 245 "unconnected-(U15-AP-Pad48)")
			(pinfunction "AP")
			(pintype "output+no_connect")
		)
		(pad "49" smd roundrect
			(at 3.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 246 "unconnected-(U15-SCLK{slash}INT2-Pad49)")
			(pinfunction "SCLK/INT2")
			(pintype "output+no_connect")
		)
		(pad "50" smd roundrect
			(at 3.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 247 "unconnected-(U15-LRCLK-Pad50)")
			(pinfunction "LRCLK")
			(pintype "output+no_connect")
		)
		(pad "51" smd roundrect
			(at 2.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 248 "unconnected-(U15-MCLK{slash}INT2-Pad51)")
			(pinfunction "MCLK/INT2")
			(pintype "output+no_connect")
		)
		(pad "52" smd roundrect
			(at 2.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "53" smd roundrect
			(at 1.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "54" smd roundrect
			(at 1.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 0.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 318 "unconnected-(U15-INT1-Pad55)")
			(pinfunction "INT1")
			(pintype "output+no_connect")
		)
		(pad "56" smd roundrect
			(at 0.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 249 "DEC_RST")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "57" smd roundrect
			(at -0.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "PVDD")
			(pintype "power_in")
		)
		(pad "58" smd roundrect
			(at -0.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "Net-(U15-XTALP)")
			(pinfunction "XTALP")
			(pintype "input")
		)
		(pad "59" smd roundrect
			(at -1.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "Net-(U15-XTALN)")
			(pinfunction "XTALN")
			(pintype "input")
		)
		(pad "60" smd roundrect
			(at -1.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "61" smd roundrect
			(at -2.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 250 "unconnected-(U15-CEC-Pad61)")
			(pinfunction "CEC")
			(pintype "bidirectional+no_connect")
		)
		(pad "62" smd roundrect
			(at -2.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 219 "/tmds_in/HDMI_SCL")
			(pinfunction "DDCA_SCL")
			(pintype "input")
		)
		(pad "63" smd roundrect
			(at -3.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 220 "/tmds_in/HDMI_SDA")
			(pinfunction "DDCA_SDA")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at -3.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 325 "+5V_HDMI")
			(pinfunction "RXA_5V")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 0 0 180)
			(size 5 5)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 120.5 99.8 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.72 105.2 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C125"
			(at -0.000003 -1.160001 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "Net-(U15-XTALN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 81.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C110"
			(at -4.8 -0.35 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 160 "/dp_in/RX2P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 161 "/dp_in/RX2PC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 90.85 32.2)
		(property "Reference" "H7"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.02 0.15 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 87.45 36.8 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D2"
			(at 2.65 -1.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.45 -0.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "+VGH")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 114.625 87.14 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at -0.06 -1.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25750"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "Net-(U20-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 123.4 105 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C179"
			(at -0.4 -1.16 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Xunpu_FPC-05F-50PH20_1x50-1MP_P0.50mm_Horizontal"
		(layer "F.Cu")
		(at 69.7 73.5 -90)
		(descr "Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
		(tags "connector Hirose FH12 horizontal")
		(property "Reference" "J6"
			(at -15.6 3.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FPC-05F-50PH20"
			(at 0 0.95 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:Xunpu_FPC-05F-50PH20_1x50-1MP_P0.50mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "\"Generic connectable mounting pin connector, single row, 01x50, script generated\""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2856813"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -12.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "-VGL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -11.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 442 "unconnected-(J6-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -11.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "+VGH")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -10.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 443 "unconnected-(J6-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -10.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 284 "-VCOM")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -9.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -9.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 287 "+5V2_FL")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -8.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "EPDC_SDOE")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -8.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "EPDC_SDLE")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -7.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "EPDC_SDCE0")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -7.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "EPDC_GDOE")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -6.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "EPDC_GDSP")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -6.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "EPDC_GDCLK")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -5.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -5.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "EPDC_SE_CLK")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -4.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -4.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "EPDC_D7N")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -3.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "EPDC_D7P")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -3.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -2.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "EPDC_D6N")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at -2.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "EPDC_D6P")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -1.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -1.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "EPDC_D5N")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -0.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "EPDC_D5P")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -0.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 0.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "EPDC_D4N")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 0.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "EPDC_D4P")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 1.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 1.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "EPDC_D3N")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 2.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "EPDC_D3P")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 2.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 3.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "EPDC_D2N")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 3.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "EPDC_D2P")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 4.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at 4.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "EPDC_D1N")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 5.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "EPDC_D1P")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at 5.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at 6.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "EPDC_D0N")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at 6.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "EPDC_D0P")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at 7.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at 7.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "FL_PWM1")
			(pinfunction "Pin_41")
			(pintype "passive")
		)
		(pad "42" smd rect
			(at 8.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "FL_PWM2")
			(pinfunction "Pin_42")
			(pintype "passive")
		)
		(pad "43" smd rect
			(at 8.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 326 "FL_EN")
			(pinfunction "Pin_43")
			(pintype "passive")
		)
		(pad "44" smd rect
			(at 9.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 287 "+5V2_FL")
			(pinfunction "Pin_44")
			(pintype "passive")
		)
		(pad "45" smd rect
			(at 9.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "Pin_45")
			(pintype "passive")
		)
		(pad "46" smd rect
			(at 10.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 441 "unconnected-(J6-Pin_46-Pad46)")
			(pinfunction "Pin_46")
			(pintype "passive+no_connect")
		)
		(pad "47" smd rect
			(at 10.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "-VN")
			(pinfunction "Pin_47")
			(pintype "passive")
		)
		(pad "48" smd rect
			(at 11.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 444 "unconnected-(J6-Pin_48-Pad48)")
			(pinfunction "Pin_48")
			(pintype "passive+no_connect")
		)
		(pad "49" smd rect
			(at 11.75 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 286 "+VP")
			(pinfunction "Pin_49")
			(pintype "passive")
		)
		(pad "50" smd rect
			(at 12.25 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 440 "unconnected-(J6-Pin_50-Pad50)")
			(pinfunction "Pin_50")
			(pintype "passive+no_connect")
		)
		(pad "MP" smd rect
			(at -13.94 0.75 270)
			(size 1.8 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 13.94 0.75 270)
			(size 2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FPC-SMD_50P-P0.50_FPC-05F-50PH20.step"
			(offset
				(xyz 0 1.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.1 38.2 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R96"
			(at -1.9 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 337 "VP_MEA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 88.8 92.4 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C73"
			(at 2.2 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 145.4 73.4 90)
		(property "Reference" "H21"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.03 0 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.68 72.94 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R109"
			(at 0 -0.88 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25105"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "Net-(X1-OUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 339 "GCLK")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
		(layer "F.Cu")
		(at 91.335 53.15 90)
		(descr "Texas RGV0016A VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/ina3221.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U21"
			(at -5.45 -3.035 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "INA3221"
			(at 0 3.33 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina3221.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Triple-Channel High-Side Shunt and Bus Voltage Monitor with I2C and SMBUS Compatible Interface, QFN-16"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C181255"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*RGV0016A*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.525 -0.525 90)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.525 0.525 90)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.525 -0.525 90)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.525 0.525 90)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.8625 -0.975 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "IN-3")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.8625 -0.325 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "IN+3")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.8625 0.325 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -1.8625 0.975 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -0.975 1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -0.325 1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 0.325 1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 0.975 1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "unconnected-(U21-WARNING-Pad8)")
			(pinfunction "WARNING")
			(pintype "open_collector+no_connect")
		)
		(pad "9" smd roundrect
			(at 1.8625 0.975 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "EPD_PWR_EN")
			(pinfunction "CRITICAL")
			(pintype "open_collector")
		)
		(pad "10" smd roundrect
			(at 1.8625 0.325 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "unconnected-(U21-PV-Pad10)")
			(pinfunction "PV")
			(pintype "open_collector+no_connect")
		)
		(pad "11" smd roundrect
			(at 1.8625 -0.325 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "+5V_ES")
			(pinfunction "IN-1")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 1.8625 -0.975 90)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pinfunction "IN+1")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 0.975 -1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 123 "unconnected-(U21-TC-Pad13)")
			(pinfunction "TC")
			(pintype "open_collector+no_connect")
		)
		(pad "14" smd roundrect
			(at 0.325 -1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 303 "+5V_EG")
			(pinfunction "IN-2")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -0.325 -1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pinfunction "IN+2")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at -0.975 -1.8625 90)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "VPU")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 90)
			(size 2.1 2.1)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "EP")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 124.62 99.5 180)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN7"
			(at 1.72 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 322 "unconnected-(RN7-R1.1-Pad1)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 254 "/tmds_in/ADV_VS")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 253 "/tmds_in/ADV_HS")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 252 "/tmds_in/ADV_DE")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 223 "DPI_DE")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 224 "DPI_HS")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 225 "DPI_VS")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 321 "unconnected-(RN7-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 94.05 46)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at -0.95 1.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 452 "/epd_power/+5V_VSH")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 134.02 105.1)
		(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y3"
			(at 2.88 -1.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "24MHz"
			(at 0 2.45 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C70590"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "Net-(U15-XTALP)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "Net-(U15-XTALN)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 137.7 64.9 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R123"
			(at -0.7 3.4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25790"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 309 "Net-(U13-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 126.2 58.2 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C90"
			(at -0.2 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 383 "Net-(C145-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 89.8 60.15)
		(property "Reference" "H9"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.04 -0.13 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108 103 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -2.6 -0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TFC-WPAPR-08"
		(layer "F.Cu")
		(at 146.4 38.75134)
		(descr "OFFSET X-> -0.950MM")
		(tags "OFFSET X-> -0.950MM")
		(property "Reference" "J7"
			(at -1.4 8.24866 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MICRO_SD(TFC-WPAPR-08)"
			(at -11.0617 -1.651 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:TFC-WPAPR-08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C91145"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 3.2512 -3.048)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 3.2512 4.953)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "1" smd rect
			(at -7.37362 -2.2479 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 291 "SDIO_DAT2")
			(pinfunction "DAT2/RES")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -7.37362 -1.14808 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 289 "SDIO_DAT3")
			(pinfunction "CD/DAT3/CS")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -7.37362 -0.04826 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "SDIO_CMD")
			(pinfunction "CMD/DI")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -7.37362 1.04902 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -7.37362 2.14884 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "SDIO_CLK")
			(pinfunction "CLK/SCLK")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -7.37362 3.24866 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -7.37362 4.34848 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 290 "SDIO_DAT0")
			(pinfunction "DAT0/DO")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -7.37362 5.4483 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 292 "SDIO_DAT1")
			(pinfunction "DAT1/RES")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -7.37362 6.54812 270)
			(size 0.6985 1.59766)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 328 "unconnected-(J7-Pad9)")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at -6.74878 7.74954 270)
			(size 1.19888 1.39954)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -6.74878 -6.84784 270)
			(size 1.59766 1.39954)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 2.84988 7.74954 270)
			(size 1.19888 2.19964)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 2.84988 -7.74954 270)
			(size 1.19888 2.19964)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/HY-TF1007B.STEP"
			(offset
				(xyz -7.25 -7.35 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 84.8 35.8 90)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D6"
			(at 2.4 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0.4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0 90)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0 90)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 93.25 43.2)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U23"
			(at -2.25 -1.4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LGS6302B5"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304071430_Legend-Si-LGS6302_C5123975.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.5A, 1.2MHz Boost DC/DC Converter, adjustable 3-60V output voltage, SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5123975"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "Net-(D15-A)")
			(pinfunction "SW")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "Net-(U23-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 452 "/epd_power/+5V_VSH")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 452 "/epd_power/+5V_VSH")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 115.425 100.32 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -0.12 1.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U5-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(U5-BS)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC"
		(layer "F.Cu")
		(at 151 63 -90)
		(descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
		(tags "SMD SMT SPST EVQPUL EVQPUC")
		(property "Reference" "SW2"
			(at 0 3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SW"
			(at 0 3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C79174"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.375 90)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0 1.375 90)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "1" smd rect
			(at -2.625 -0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "KEY2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 2.625 -0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "KEY2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.625 0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.625 0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/EVQPU-LC-02K.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(footprint "footprints:HDMI_C_GT-HD006A-CGNGX"
		(layer "F.Cu")
		(at 153 101 90)
		(property "Reference" "J4"
			(at -5 -5.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HDMI_C_1.3"
			(at 1.715 10 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:HDMI_C_GT-HD006A-CGNGX"
			(at 0 -2.615 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://pinoutguide.com/PortableDevices/mini_hdmi_pinout.shtml"
			(at 0 -2.615 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "HDMI 1.3+ type C connector"
			(at 0 -2.615 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C27636755"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "HDMI*C*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -4.7 -3.9 90)
			(size 0.95 0.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 4.7 -3.9 90)
			(size 0.95 0.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "1" smd rect
			(at 3.6 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "D2S")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at 3.2 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 214 "/tmds_in/TMDS_D2P")
			(pinfunction "D2+")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.8 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "/tmds_in/TMDS_D2N")
			(pinfunction "D2-")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.4 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "D1S")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 183 "/tmds_in/TMDS_D1P")
			(pinfunction "D1+")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.6 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "/tmds_in/TMDS_D1N")
			(pinfunction "D1-")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.2 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "D0S")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 0.8 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "/tmds_in/TMDS_D0P")
			(pinfunction "D0+")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.4 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "/tmds_in/TMDS_D0N")
			(pinfunction "D0-")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "CKS")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at -0.4 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "/tmds_in/TMDS_CKP")
			(pinfunction "CK+")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -0.8 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "/tmds_in/TMDS_CKN")
			(pinfunction "CK-")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -1.2 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at -1.6 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "unconnected-(J4-CEC-Pad14)")
			(pinfunction "CEC")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd rect
			(at -2 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 219 "/tmds_in/HDMI_SCL")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -2.4 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 220 "/tmds_in/HDMI_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -2.8 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "unconnected-(J4-UTILITY-Pad17)")
			(pinfunction "UTILITY")
			(pintype "passive+no_connect")
		)
		(pad "18" smd rect
			(at -3.2 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 325 "+5V_HDMI")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at -3.6 -4.75 90)
			(size 0.23 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 222 "/tmds_in/HDMI_HPD")
			(pinfunction "HPD")
			(pintype "passive")
		)
		(pad "SH" thru_hole oval
			(at -6.825 0 90)
			(size 1.25 2)
			(drill oval 0.65 1.4)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at -6.81 -3.6 90)
			(size 1.75 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" smd rect
			(at 6.81 -3.6 90)
			(size 1.75 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(pad "SH" thru_hole oval
			(at 6.825 0 90)
			(size 1.25 2)
			(drill oval 0.65 1.4)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SH")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/HDMI-SMD_GT-HD006B-CGNG0.step"
			(offset
				(xyz -0.23 2.16 -3.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 128.05 108.5)
		(property "Reference" "H18"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
		(layer "F.Cu")
		(at 117.425 92.2875 180)
		(descr "Texas RGV0016A VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/ina3221.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "Texas VQFN NoLead")
		(property "Reference" "U22"
			(at 0 3.3 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "INA3221"
			(at 0 3.33 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ina3221.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Triple-Channel High-Side Shunt and Bus Voltage Monitor with I2C and SMBUS Compatible Interface, QFN-16"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C181255"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Texas*RGV0016A*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.525 -0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.525 0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.525 -0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.525 0.525 180)
			(size 0.85 0.85)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.8625 -0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 287 "+5V2_FL")
			(pinfunction "IN-3")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.8625 -0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pinfunction "IN+3")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.8625 0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -1.8625 0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -0.975 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -0.325 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 0.325 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 0.975 1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 283 "unconnected-(U22-WARNING-Pad8)")
			(pinfunction "WARNING")
			(pintype "open_collector+no_connect")
		)
		(pad "9" smd roundrect
			(at 1.8625 0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 293 "unconnected-(U22-CRITICAL-Pad9)")
			(pinfunction "CRITICAL")
			(pintype "open_collector+no_connect")
		)
		(pad "10" smd roundrect
			(at 1.8625 0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 142 "unconnected-(U22-PV-Pad10)")
			(pinfunction "PV")
			(pintype "open_collector+no_connect")
		)
		(pad "11" smd roundrect
			(at 1.8625 -0.325 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "IN-1")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 1.8625 -0.975 180)
			(size 1.025 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 307 "+1V8_DCDC")
			(pinfunction "IN+1")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 0.975 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 137 "unconnected-(U22-TC-Pad13)")
			(pinfunction "TC")
			(pintype "open_collector+no_connect")
		)
		(pad "14" smd roundrect
			(at 0.325 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pinfunction "IN-2")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -0.325 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "IN+2")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at -0.975 -1.8625 180)
			(size 0.35 1.025)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pinfunction "VPU")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 2.1 2.1)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "EP")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.55 35.65 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -0.05 -1.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 369 "/mcu/OSC32_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.2 42.32 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at 0 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-6"
		(layer "F.Cu")
		(at 117.525 103.11)
		(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U5"
			(at 2.875 2.49 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SY8113C"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6338414"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT*23*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(U5-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U5-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U5-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 141.52 92.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C135"
			(at -1.12 -2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 123.1 70.2 135)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C121"
			(at 1.414214 -0.989949 -45)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 16.25 11.37925 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 135)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "Net-(C118-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 135)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 80.05 46.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 2.05 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "240K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C64043"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U9-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100.6 82)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C69"
			(at 0 -1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 98.85 34.8 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C176"
			(at -2.15 1.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 107.7 99.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C155"
			(at 0 -1.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 300 "+1V35_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 117.625 83)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L1"
			(at -0.025 -2.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 280 "Net-(U20-SW)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 307 "+1V8_DCDC")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 87.7 47.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 1.8 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U24-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 329 "VGH_DAC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 141.6 66.2 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C97"
			(at -0.1 2.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.3 69.8 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C102"
			(at 0 -3.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 310 "Net-(U13-VIN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 142 106.4)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at -1 1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 457 "Net-(U10-VOUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 222 "/tmds_in/HDMI_HPD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-6"
		(layer "F.Cu")
		(at 82.05 43.2)
		(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U9"
			(at -2.6 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LGS5145"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5123971"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT*23*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(U9-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U9-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "/epd_power/EN_VGL")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 303 "+5V_EG")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 458 "Net-(D3-K)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 83.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at -4.6 -0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "/dp_in/TX1P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "/dp_in/TX1PC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.1 102.4 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 300 "+1V35_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "Net-(U2-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 101.5 56.25)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D1"
			(at -2.4 2.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0.35 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 131.32 105.1 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C113"
			(at -0.45 -0.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "Net-(U15-XTALP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 128.35 61.5)
		(property "Reference" "H17"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.02 0.01 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Package_BGA:WLP-4_0.83x0.83mm_P0.4mm"
		(layer "F.Cu")
		(at 93.6 48.5 -90)
		(descr "WLP-4_0.83x0.83mm_P0.4mm https://pdfserv.maximintegrated.com/package_dwgs/21-100107.PDF, https://www.maximintegrated.com/en/app-notes/index.mvp/id/1891")
		(tags "WLP-4")
		(property "Reference" "U7"
			(at 0.2 -3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS22914BYFPR"
			(at 0 2.25 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_BGA:WLP-4_0.83x0.83mm_P0.4mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22913.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Slew rate controlled load switch, WLCSP-4"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1848394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WLCSP*X1*WLB0909*0.89x0.89*P0.5mm*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -0.2 -0.2 270)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 452 "/epd_power/+5V_VSH")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "A2" smd circle
			(at 0.2 -0.2 270)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 302 "+5V_ES")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "B1" smd circle
			(at -0.2 0.2 270)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B2" smd circle
			(at 0.2 0.2 270)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 221 "EPD_POS_EN")
			(pinfunction "ON")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_BGA.3dshapes/WLP-4_0.83x0.83mm_P0.4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 111.4 67 90)
		(property "Reference" "H19"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.01 -0.05 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:BGA-96_9.0x14.0mm_P0.8mm"
		(layer "F.Cu")
		(at 88.65 98.67 -90)
		(descr "BGA-96, http://www.mouser.com/ds/2/198/43-46TR16640B-81280BL-706483.pdf")
		(tags "BGA-96")
		(property "Reference" "U12"
			(at 0 -7.75 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MT41K64M16TW"
			(at 0 7.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:BGA-96_9.0x14.0mm_P0.8mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C524855"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "3.2405"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -3.2 -6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "A2" smd circle
			(at -2.4 -6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/fpga_ddr/DRAM_DATA13")
			(pinfunction "DQ13")
			(pintype "bidirectional")
		)
		(pad "A3" smd circle
			(at -1.6 -6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "/fpga_ddr/DRAM_DATA15")
			(pinfunction "DQ15")
			(pintype "bidirectional")
		)
		(pad "A7" smd circle
			(at 1.6 -6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/fpga_ddr/DRAM_DATA12")
			(pinfunction "DQ12")
			(pintype "bidirectional")
		)
		(pad "A8" smd circle
			(at 2.4 -6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "A9" smd circle
			(at 3.2 -6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "B1" smd circle
			(at -3.2 -5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "B2" smd circle
			(at -2.4 -5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "B3" smd circle
			(at -1.6 -5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "B7" smd circle
			(at 1.6 -5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 376 "/fpga_ddr/DRAM_UDQSN")
			(pinfunction "~{UDQS}")
			(pintype "input")
		)
		(pad "B8" smd circle
			(at 2.4 -5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/fpga_ddr/DRAM_DATA14")
			(pinfunction "DQ14")
			(pintype "bidirectional")
		)
		(pad "B9" smd circle
			(at 3.2 -5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "C1" smd circle
			(at -3.2 -4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "C2" smd circle
			(at -2.4 -4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/fpga_ddr/DRAM_DATA11")
			(pinfunction "DQ11")
			(pintype "bidirectional")
		)
		(pad "C3" smd circle
			(at -1.6 -4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "/fpga_ddr/DRAM_DATA9")
			(pinfunction "DQ9")
			(pintype "bidirectional")
		)
		(pad "C7" smd circle
			(at 1.6 -4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 385 "/fpga_ddr/DRAM_UDQSP")
			(pinfunction "UDQS")
			(pintype "bidirectional")
		)
		(pad "C8" smd circle
			(at 2.4 -4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/fpga_ddr/DRAM_DATA10")
			(pinfunction "DQ10")
			(pintype "bidirectional")
		)
		(pad "C9" smd circle
			(at 3.2 -4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "D1" smd circle
			(at -3.2 -3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "D2" smd circle
			(at -2.4 -3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "D3" smd circle
			(at -1.6 -3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 394 "/fpga_ddr/DRAM_UDM")
			(pinfunction "UDM")
			(pintype "input")
		)
		(pad "D7" smd circle
			(at 1.6 -3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/fpga_ddr/DRAM_DATA8")
			(pinfunction "DQ8")
			(pintype "bidirectional")
		)
		(pad "D8" smd circle
			(at 2.4 -3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "D9" smd circle
			(at 3.2 -3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "E1" smd circle
			(at -3.2 -2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "E2" smd circle
			(at -2.4 -2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "E3" smd circle
			(at -1.6 -2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/fpga_ddr/DRAM_DATA0")
			(pinfunction "DQ0")
			(pintype "bidirectional")
		)
		(pad "E7" smd circle
			(at 1.6 -2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 397 "/fpga_ddr/DRAM_LDM")
			(pinfunction "LDM")
			(pintype "input")
		)
		(pad "E8" smd circle
			(at 2.4 -2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "E9" smd circle
			(at 3.2 -2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -3.2 -2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "F2" smd circle
			(at -2.4 -2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/fpga_ddr/DRAM_DATA2")
			(pinfunction "DQ2")
			(pintype "bidirectional")
		)
		(pad "F3" smd circle
			(at -1.6 -2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 390 "/fpga_ddr/DRAM_LDQSP")
			(pinfunction "LDQS")
			(pintype "input")
		)
		(pad "F7" smd circle
			(at 1.6 -2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "/fpga_ddr/DRAM_DATA1")
			(pinfunction "DQ1")
			(pintype "bidirectional")
		)
		(pad "F8" smd circle
			(at 2.4 -2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/fpga_ddr/DRAM_DATA3")
			(pinfunction "DQ3")
			(pintype "bidirectional")
		)
		(pad "F9" smd circle
			(at 3.2 -2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "G1" smd circle
			(at -3.2 -1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "G2" smd circle
			(at -2.4 -1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "/fpga_ddr/DRAM_DATA6")
			(pinfunction "DQ6")
			(pintype "bidirectional")
		)
		(pad "G3" smd circle
			(at -1.6 -1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 389 "/fpga_ddr/DRAM_LDQSN")
			(pinfunction "~{LDQS}")
			(pintype "input")
		)
		(pad "G7" smd circle
			(at 1.6 -1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "G8" smd circle
			(at 2.4 -1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "G9" smd circle
			(at 3.2 -1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "H1" smd circle
			(at -3.2 -0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+DRAM_VREF")
			(pinfunction "VrefDQ")
			(pintype "power_in")
		)
		(pad "H2" smd circle
			(at -2.4 -0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "H3" smd circle
			(at -1.6 -0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "/fpga_ddr/DRAM_DATA4")
			(pinfunction "DQ4")
			(pintype "bidirectional")
		)
		(pad "H7" smd circle
			(at 1.6 -0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/fpga_ddr/DRAM_DATA7")
			(pinfunction "DQ7")
			(pintype "bidirectional")
		)
		(pad "H8" smd circle
			(at 2.4 -0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/fpga_ddr/DRAM_DATA5")
			(pinfunction "DQ5")
			(pintype "bidirectional")
		)
		(pad "H9" smd circle
			(at 3.2 -0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "J1" smd circle
			(at -3.2 0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "J2" smd circle
			(at -2.4 0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "J3" smd circle
			(at -1.6 0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/fpga_ddr/DRAM_RASB")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "J7" smd circle
			(at 1.6 0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/fpga_ddr/DRAM_CKP")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "J8" smd circle
			(at 2.4 0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "J9" smd circle
			(at 3.2 0.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "K1" smd circle
			(at -3.2 1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "/fpga_ddr/DRAM_ODT")
			(pinfunction "ODT")
			(pintype "input")
		)
		(pad "K2" smd circle
			(at -2.4 1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "K3" smd circle
			(at -1.6 1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/fpga_ddr/DRAM_CASB")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "K7" smd circle
			(at 1.6 1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/fpga_ddr/DRAM_CKN")
			(pinfunction "~{CK}")
			(pintype "input")
		)
		(pad "K8" smd circle
			(at 2.4 1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "K9" smd circle
			(at 3.2 1.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "/fpga_ddr/DRAM_CKE")
			(pinfunction "CKE")
			(pintype "input")
		)
		(pad "L1" smd circle
			(at -3.2 2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "L2" smd circle
			(at -2.4 2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/fpga_ddr/DRAM_CSB")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "L3" smd circle
			(at -1.6 2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/fpga_ddr/DRAM_WEB")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "L7" smd circle
			(at 1.6 2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/fpga_ddr/DRAM_ADDR10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "L8" smd circle
			(at 2.4 2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 338 "Net-(U12-ZQ)")
			(pinfunction "ZQ")
			(pintype "input")
		)
		(pad "L9" smd circle
			(at 3.2 2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "M1" smd circle
			(at -3.2 2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "M2" smd circle
			(at -2.4 2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/fpga_ddr/DRAM_BA0")
			(pinfunction "BA0")
			(pintype "input")
		)
		(pad "M3" smd circle
			(at -1.6 2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/fpga_ddr/DRAM_BA2")
			(pinfunction "BA2")
			(pintype "input")
		)
		(pad "M7" smd circle
			(at 1.6 2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 422 "unconnected-(U12-A15{slash}NC-PadM7)")
			(pinfunction "A15/NC")
			(pintype "input+no_connect")
		)
		(pad "M8" smd circle
			(at 2.4 2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+DRAM_VREF")
			(pinfunction "VrefCA")
			(pintype "power_in")
		)
		(pad "M9" smd circle
			(at 3.2 2.8 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "N1" smd circle
			(at -3.2 3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "N2" smd circle
			(at -2.4 3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/fpga_ddr/DRAM_ADDR3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "N3" smd circle
			(at -1.6 3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/fpga_ddr/DRAM_ADDR0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "N7" smd circle
			(at 1.6 3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/fpga_ddr/DRAM_ADDR12")
			(pinfunction "A12/~{BC}")
			(pintype "input")
		)
		(pad "N8" smd circle
			(at 2.4 3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/fpga_ddr/DRAM_BA1")
			(pinfunction "BA1")
			(pintype "input")
		)
		(pad "N9" smd circle
			(at 3.2 3.6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "P1" smd circle
			(at -3.2 4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "P2" smd circle
			(at -2.4 4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "/fpga_ddr/DRAM_ADDR5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "P3" smd circle
			(at -1.6 4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/fpga_ddr/DRAM_ADDR2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "P7" smd circle
			(at 1.6 4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/fpga_ddr/DRAM_ADDR1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "P8" smd circle
			(at 2.4 4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "/fpga_ddr/DRAM_ADDR4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "P9" smd circle
			(at 3.2 4.4 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "R1" smd circle
			(at -3.2 5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "R2" smd circle
			(at -2.4 5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/fpga_ddr/DRAM_ADDR7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "R3" smd circle
			(at -1.6 5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/fpga_ddr/DRAM_ADDR9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "R7" smd circle
			(at 1.6 5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "/fpga_ddr/DRAM_ADDR11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "R8" smd circle
			(at 2.4 5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/fpga_ddr/DRAM_ADDR6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "R9" smd circle
			(at 3.2 5.2 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "T1" smd circle
			(at -3.2 6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "T2" smd circle
			(at -2.4 6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/fpga_ddr/DRAM_RST")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "T3" smd circle
			(at -1.6 6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/fpga_ddr/DRAM_ADDR13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "T7" smd circle
			(at 1.6 6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/fpga_ddr/DRAM_ADDR14")
			(pinfunction "A14/NC")
			(pintype "input")
		)
		(pad "T8" smd circle
			(at 2.4 6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "/fpga_ddr/DRAM_ADDR8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "T9" smd circle
			(at 3.2 6 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_BGA.3dshapes/BGA-96_9.0x13.0mm_Layout2x3x16_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 115.225 83.9 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C153"
			(at -2.3 0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 280 "Net-(U20-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 279 "Net-(U20-BS)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.2 46.3 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at -1.3 0.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 284 "-VCOM")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 79.45 41.6 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 458 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "Net-(U9-BS)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 108 90.7125)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C141"
			(at 0.4 1.0875 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 127.7 80.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C120"
			(at 2.5 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at -9.975841 -15.655672 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "Net-(C117-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 58.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C169"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "VGL_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 125.2 69.02 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB2"
			(at -0.02 1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100M"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14709"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "Net-(C118-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 117.825 99.4)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L2"
			(at -2.6 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U5-SW)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 299 "+3V3_DCDC")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 136.22 87.4 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN11"
			(at 1.75 0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 270 "/tmds_in/ADV_P16")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 267 "/tmds_in/ADV_P17")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 269 "/tmds_in/ADV_P18")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 268 "/tmds_in/ADV_P19")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 237 "DPI_R3")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 238 "DPI_R2")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 344 "unconnected-(RN11-R2.2-Pad7)")
			(pinfunction "R2.2")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 343 "unconnected-(RN11-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 81.95 56.8 -90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U6"
			(at 1 2.2 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MT9700"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C89855"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(U6-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "EPD_PWR_EN")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 134.47 87.4 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C128"
			(at 2.6 -0.87 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 120.95 60.2)
		(property "Reference" "H23"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -0.01 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_TXC_9HT11-2Pin_2.0x1.2mm_HandSoldering"
		(layer "F.Cu")
		(at 127 36.075 90)
		(descr "SMD Crystal TXC 9HT11 http://txccrystal.com/images/pdf/9ht11.pdf, hand-soldering, 2.0x1.2mm^2 package")
		(tags "SMD SMT crystal hand-soldering")
		(property "Reference" "Y2"
			(at 3.275 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "32.768K"
			(at 0 1.8 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Crystal:Crystal_SMD_TXC_9HT11-2Pin_2.0x1.2mm_HandSoldering"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7500573"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.925 0 90)
			(size 1.05 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 368 "/mcu/OSC32_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.925 0 90)
			(size 1.05 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 369 "/mcu/OSC32_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_TXC_9HT11-2Pin_2.0x1.2mm_HandSoldering.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 105.0125 45.15 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q6"
			(at 0 -3.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AO3400A"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C347475"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "Net-(Q6-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(Q6-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 284 "-VCOM")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 127.2 58.2 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C145"
			(at -0.2 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 383 "Net-(C145-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 96 104.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C85"
			(at 0 1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0301"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93.4 104.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C82"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 93.8 108.5)
		(property "Reference" "H12"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -0.02 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120.4 38.1 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at -1.9 0.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 371 "Net-(U3-NRST)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 137.9 106 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -0.05 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 219 "/tmds_in/HDMI_SCL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 325 "+5V_HDMI")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 118.9 38.1 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 1.9 -0.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 374 "+3V3A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Xilinx_FTG256"
		(layer "F.Cu")
		(at 90.5 75.9 90)
		(descr "Artix-7 BGA, 16x16 grid, 17x17mm package, 1mm pitch; https://www.xilinx.com/support/documentation/user_guides/ug475_7Series_Pkg_Pinout.pdf#page=269, NSMD pad definition Appendix A")
		(tags "BGA 256 1 FT256 FTG256")
		(property "Reference" "U1"
			(at 0 -9.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "XC6SLX-FTG256"
			(at 0 9.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:Xilinx_FTG256"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Spartan 6 LX 16 XC6SLX16-FTG256"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C39313"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(solder_mask_margin 0.05)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -7.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A2" smd circle
			(at -6.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/fpga_ddr/DRAM_ADDR9")
			(pinfunction "IO_L52N_M3A9_3")
			(pintype "bidirectional")
		)
		(pad "A3" smd circle
			(at -5.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+DRAM_VREF")
			(pinfunction "IO_L83N_VREF_3")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at -4.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 429 "unconnected-(U1A-IO_L1N_VREF_0-PadA4)")
			(pinfunction "IO_L1N_VREF_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "A5" smd circle
			(at -3.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 432 "unconnected-(U1A-IO_L2N_0-PadA5)")
			(pinfunction "IO_L2N_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "A6" smd circle
			(at -2.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 431 "unconnected-(U1A-IO_L4N_0-PadA6)")
			(pinfunction "IO_L4N_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "A7" smd circle
			(at -1.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "EPDC_D8N")
			(pinfunction "IO_L6N_0")
			(pintype "bidirectional")
		)
		(pad "A8" smd circle
			(at -0.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "EPDC_D10P")
			(pinfunction "IO_L33N_0")
			(pintype "bidirectional")
		)
		(pad "A9" smd circle
			(at 0.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "EPDC_D11P")
			(pinfunction "IO_L34N_GCLK18_0")
			(pintype "bidirectional")
		)
		(pad "A10" smd circle
			(at 1.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "EPDC_D1P")
			(pinfunction "IO_L35N_GCLK16_0")
			(pintype "bidirectional")
		)
		(pad "A11" smd circle
			(at 2.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "EPDC_D4P")
			(pinfunction "IO_L39N_0")
			(pintype "bidirectional")
		)
		(pad "A12" smd circle
			(at 3.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "EPDC_D5P")
			(pinfunction "IO_L62N_VREF_0")
			(pintype "bidirectional")
		)
		(pad "A13" smd circle
			(at 4.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "EPDC_D6P")
			(pinfunction "IO_L63N_SCP6_0")
			(pintype "bidirectional")
		)
		(pad "A14" smd circle
			(at 5.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "EPDC_D7P")
			(pinfunction "IO_L65N_SCP2_0")
			(pintype "bidirectional")
		)
		(pad "A15" smd circle
			(at 6.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "FPGA_TMS")
			(pinfunction "TMS")
			(pintype "bidirectional")
		)
		(pad "A16" smd circle
			(at 7.5 -7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B1" smd circle
			(at -7.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/fpga_ddr/DRAM_BA2")
			(pinfunction "IO_L50N_M3BA2_3")
			(pintype "bidirectional")
		)
		(pad "B2" smd circle
			(at -6.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "/fpga_ddr/DRAM_ADDR8")
			(pinfunction "IO_L52P_M3A8_3")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at -5.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 373 "unconnected-(U1D-IO_L83P_3-PadB3)")
			(pinfunction "IO_L83P_3")
			(pintype "bidirectional")
		)
		(pad "B4" smd circle
			(at -4.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_0")
			(pintype "power_in")
		)
		(pad "B5" smd circle
			(at -3.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 423 "unconnected-(U1A-IO_L2P_0-PadB5)")
			(pinfunction "IO_L2P_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "B6" smd circle
			(at -2.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 424 "unconnected-(U1A-IO_L4P_0-PadB6)")
			(pinfunction "IO_L4P_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "B7" smd circle
			(at -1.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B8" smd circle
			(at -0.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "EPDC_D10N")
			(pinfunction "IO_L33P_0")
			(pintype "bidirectional")
		)
		(pad "B9" smd circle
			(at 0.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_0")
			(pintype "power_in")
		)
		(pad "B10" smd circle
			(at 1.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "EPDC_D1N")
			(pinfunction "IO_L35P_GCLK17_0")
			(pintype "bidirectional")
		)
		(pad "B11" smd circle
			(at 2.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B12" smd circle
			(at 3.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "EPDC_D5N")
			(pinfunction "IO_L62P_0")
			(pintype "bidirectional")
		)
		(pad "B13" smd circle
			(at 4.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_0")
			(pintype "power_in")
		)
		(pad "B14" smd circle
			(at 5.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "EPDC_D7N")
			(pinfunction "IO_L65P_SCP3_0")
			(pintype "bidirectional")
		)
		(pad "B15" smd circle
			(at 6.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "EPDC_SE_CLK")
			(pinfunction "IO_L29P_A23_M1A13_1")
			(pintype "bidirectional")
		)
		(pad "B16" smd circle
			(at 7.5 -6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "EPDC_GDCLK")
			(pinfunction "IO_L29N_A22_M1A14_1")
			(pintype "bidirectional")
		)
		(pad "C1" smd circle
			(at -7.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/fpga_ddr/DRAM_WEB")
			(pinfunction "IO_L50P_M3WE_3")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -6.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/fpga_ddr/DRAM_BA1")
			(pinfunction "IO_L48N_M3BA1_3")
			(pintype "bidirectional")
		)
		(pad "C3" smd circle
			(at -5.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/fpga_ddr/DRAM_BA0")
			(pinfunction "IO_L48P_M3BA0_3")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at -4.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 426 "unconnected-(U1A-IO_L1P_HSWAPEN_0-PadC4)")
			(pinfunction "IO_L1P_HSWAPEN_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "C5" smd circle
			(at -3.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 433 "unconnected-(U1A-IO_L3N_0-PadC5)")
			(pinfunction "IO_L3N_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "C6" smd circle
			(at -2.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "unconnected-(U1A-IO_L7N_0-PadC6)")
			(pinfunction "IO_L7N_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "C7" smd circle
			(at -1.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "EPDC_D8P")
			(pinfunction "IO_L6P_0")
			(pintype "bidirectional")
		)
		(pad "C8" smd circle
			(at -0.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "EPDC_CLKP")
			(pinfunction "IO_L38N_VREF_0")
			(pintype "bidirectional")
		)
		(pad "C9" smd circle
			(at 0.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "EPDC_D11N")
			(pinfunction "IO_L34P_GCLK19_0")
			(pintype "bidirectional")
		)
		(pad "C10" smd circle
			(at 1.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "EPDC_D0N")
			(pinfunction "IO_L37N_GCLK12_0")
			(pintype "bidirectional")
		)
		(pad "C11" smd circle
			(at 2.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "EPDC_D4N")
			(pinfunction "IO_L39P_0")
			(pintype "bidirectional")
		)
		(pad "C12" smd circle
			(at 3.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "FPGA_TDI")
			(pinfunction "TDI")
			(pintype "bidirectional")
		)
		(pad "C13" smd circle
			(at 4.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "EPDC_D6N")
			(pinfunction "IO_L63P_SCP7_0")
			(pintype "bidirectional")
		)
		(pad "C14" smd circle
			(at 5.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "FPGA_TCK")
			(pinfunction "TCK")
			(pintype "bidirectional")
		)
		(pad "C15" smd circle
			(at 6.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 144 "/fpga_io/LED")
			(pinfunction "IO_L33P_A15_M1A10_1")
			(pintype "bidirectional")
		)
		(pad "C16" smd circle
			(at 7.5 -5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "EPDC_GDSP")
			(pinfunction "IO_L33N_A14_M1A4_1")
			(pintype "bidirectional")
		)
		(pad "D1" smd circle
			(at -7.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/fpga_ddr/DRAM_ADDR2")
			(pinfunction "IO_L49N_M3A2_3")
			(pintype "bidirectional")
		)
		(pad "D2" smd circle
			(at -6.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VCCO_3")
			(pintype "power_in")
		)
		(pad "D3" smd circle
			(at -5.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/fpga_ddr/DRAM_ADDR7")
			(pinfunction "IO_L49P_M3A7_3")
			(pintype "bidirectional")
		)
		(pad "D4" smd circle
			(at -4.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "D5" smd circle
			(at -3.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 434 "unconnected-(U1A-IO_L3P_0-PadD5)")
			(pinfunction "IO_L3P_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "D6" smd circle
			(at -2.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 430 "unconnected-(U1A-IO_L7P_0-PadD6)")
			(pinfunction "IO_L7P_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "D7" smd circle
			(at -1.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_0")
			(pintype "power_in")
		)
		(pad "D8" smd circle
			(at -0.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "EPDC_CLKN")
			(pinfunction "IO_L38P_0")
			(pintype "bidirectional")
		)
		(pad "D9" smd circle
			(at 0.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 435 "unconnected-(U1A-IO_L40N_0-PadD9)")
			(pinfunction "IO_L40N_0")
			(pintype "bidirectional")
		)
		(pad "D10" smd circle
			(at 1.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_0")
			(pintype "power_in")
		)
		(pad "D11" smd circle
			(at 2.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "EPDC_D3P")
			(pinfunction "IO_L66P_SCP1_0")
			(pintype "bidirectional")
		)
		(pad "D12" smd circle
			(at 3.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "EPDC_D3N")
			(pinfunction "IO_L66N_SCP0_0")
			(pintype "bidirectional")
		)
		(pad "D13" smd circle
			(at 4.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "D14" smd circle
			(at 5.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 233 "DPI_R7")
			(pinfunction "IO_L31P_A19_M1CKE_1")
			(pintype "bidirectional")
		)
		(pad "D15" smd circle
			(at 6.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_1")
			(pintype "power_in")
		)
		(pad "D16" smd circle
			(at 7.5 -4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "EPDC_GDOE")
			(pinfunction "IO_L31N_A18_M1A12_1")
			(pintype "bidirectional")
		)
		(pad "E1" smd circle
			(at -7.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/fpga_ddr/DRAM_CKN")
			(pinfunction "IO_L46N_M3CLKN_3")
			(pintype "bidirectional")
		)
		(pad "E2" smd circle
			(at -6.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/fpga_ddr/DRAM_CKP")
			(pinfunction "IO_L46P_M3CLK_3")
			(pintype "bidirectional")
		)
		(pad "E3" smd circle
			(at -5.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "/fpga_ddr/DRAM_ADDR11")
			(pinfunction "IO_L54N_M3A11_3")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at -4.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/fpga_ddr/DRAM_RST")
			(pinfunction "IO_L54P_M3RESET_3")
			(pintype "bidirectional")
		)
		(pad "E5" smd circle
			(at -3.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "E6" smd circle
			(at -2.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 427 "unconnected-(U1A-IO_L5N_0-PadE6)")
			(pinfunction "IO_L5N_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "E7" smd circle
			(at -1.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "EPDC_D9P")
			(pinfunction "IO_L36P_GCLK15_0")
			(pintype "bidirectional")
		)
		(pad "E8" smd circle
			(at -0.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "EPDC_D9N")
			(pinfunction "IO_L36N_GCLK14_0")
			(pintype "bidirectional")
		)
		(pad "E9" smd circle
			(at 0.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "E10" smd circle
			(at 1.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "EPDC_D0P")
			(pinfunction "IO_L37P_GCLK13_0")
			(pintype "bidirectional")
		)
		(pad "E11" smd circle
			(at 2.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "EPDC_D2N")
			(pinfunction "IO_L64N_SCP4_0")
			(pintype "bidirectional")
		)
		(pad "E12" smd circle
			(at 3.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 352 "unconnected-(U1B-IO_L1N_A24_VREF_1-PadE12)")
			(pinfunction "IO_L1N_A24_VREF_1")
			(pintype "bidirectional")
		)
		(pad "E13" smd circle
			(at 4.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 438 "unconnected-(U1B-IO_L1P_A25_1-PadE13)")
			(pinfunction "IO_L1P_A25_1")
			(pintype "bidirectional")
		)
		(pad "E14" smd circle
			(at 5.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "FPGA_TDO")
			(pinfunction "TDO")
			(pintype "bidirectional")
		)
		(pad "E15" smd circle
			(at 6.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "EPDC_SDCE0")
			(pinfunction "IO_L34P_A13_M1WE_1")
			(pintype "bidirectional")
		)
		(pad "E16" smd circle
			(at 7.5 -3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "EPDC_SDLE")
			(pinfunction "IO_L34N_A12_M1BA2_1")
			(pintype "bidirectional")
		)
		(pad "F1" smd circle
			(at -7.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/fpga_ddr/DRAM_DATA5")
			(pinfunction "IO_L41N_GCLK26_M3DQ5_3")
			(pintype "bidirectional")
		)
		(pad "F2" smd circle
			(at -6.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "/fpga_ddr/DRAM_DATA4")
			(pinfunction "IO_L41P_GCLK27_M3DQ4_3")
			(pintype "bidirectional")
		)
		(pad "F3" smd circle
			(at -5.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/fpga_ddr/DRAM_ADDR12")
			(pinfunction "IO_L53N_M3A12_3")
			(pintype "bidirectional")
		)
		(pad "F4" smd circle
			(at -4.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "/fpga_ddr/DRAM_CKE")
			(pinfunction "IO_L53P_M3CKE_3")
			(pintype "bidirectional")
		)
		(pad "F5" smd circle
			(at -3.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/fpga_ddr/DRAM_ADDR14")
			(pinfunction "IO_L55N_M3A14_3")
			(pintype "bidirectional")
		)
		(pad "F6" smd circle
			(at -2.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/fpga_ddr/DRAM_ADDR13")
			(pinfunction "IO_L55P_M3A13_3")
			(pintype "bidirectional")
		)
		(pad "F7" smd circle
			(at -1.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 425 "unconnected-(U1A-IO_L5P_0-PadF7)")
			(pinfunction "IO_L5P_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "F8" smd circle
			(at -0.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "F9" smd circle
			(at 0.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 436 "unconnected-(U1A-IO_L40P_0-PadF9)")
			(pinfunction "IO_L40P_0")
			(pintype "bidirectional")
		)
		(pad "F10" smd circle
			(at 1.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "EPDC_D2P")
			(pinfunction "IO_L64P_SCP5_0")
			(pintype "bidirectional")
		)
		(pad "F11" smd circle
			(at 2.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "F12" smd circle
			(at 3.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 375 "unconnected-(U1B-IO_L30P_A21_M1RESET_1-PadF12)")
			(pinfunction "IO_L30P_A21_M1RESET_1")
			(pintype "bidirectional")
		)
		(pad "F13" smd circle
			(at 4.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 364 "unconnected-(U1B-IO_L32P_A17_M1A8_1-PadF13)")
			(pinfunction "IO_L32P_A17_M1A8_1")
			(pintype "bidirectional")
		)
		(pad "F14" smd circle
			(at 5.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 437 "unconnected-(U1B-IO_L32N_A16_M1A9_1-PadF14)")
			(pinfunction "IO_L32N_A16_M1A9_1")
			(pintype "bidirectional")
		)
		(pad "F15" smd circle
			(at 6.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "EPDC_SDOE")
			(pinfunction "IO_L35P_A11_M1A7_1")
			(pintype "bidirectional")
		)
		(pad "F16" smd circle
			(at 7.5 -2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 418 "FMC_D2")
			(pinfunction "IO_L35N_A10_M1A2_1")
			(pintype "bidirectional")
		)
		(pad "G1" smd circle
			(at -7.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/fpga_ddr/DRAM_DATA7")
			(pinfunction "IO_L40N_M3DQ7_3")
			(pintype "bidirectional")
		)
		(pad "G2" smd circle
			(at -6.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "G3" smd circle
			(at -5.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "/fpga_ddr/DRAM_DATA6")
			(pinfunction "IO_L40P_M3DQ6_3")
			(pintype "bidirectional")
		)
		(pad "G4" smd circle
			(at -4.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VCCO_3")
			(pintype "power_in")
		)
		(pad "G5" smd circle
			(at -3.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "/fpga_ddr/DRAM_ADDR4")
			(pinfunction "IO_L51N_M3A4_3")
			(pintype "bidirectional")
		)
		(pad "G6" smd circle
			(at -2.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/fpga_ddr/DRAM_ADDR10")
			(pinfunction "IO_L51P_M3A10_3")
			(pintype "bidirectional")
		)
		(pad "G7" smd circle
			(at -1.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "G8" smd circle
			(at -0.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "G9" smd circle
			(at 0.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "G10" smd circle
			(at 1.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "G11" smd circle
			(at 2.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 370 "unconnected-(U1B-IO_L30N_A20_M1A11_1-PadG11)")
			(pinfunction "IO_L30N_A20_M1A11_1")
			(pintype "bidirectional")
		)
		(pad "G12" smd circle
			(at 3.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 235 "DPI_R5")
			(pinfunction "IO_L38P_A5_M1CLK_1")
			(pintype "bidirectional")
		)
		(pad "G13" smd circle
			(at 4.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_1")
			(pintype "power_in")
		)
		(pad "G14" smd circle
			(at 5.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 234 "DPI_R6")
			(pinfunction "IO_L36P_A9_M1BA0_1")
			(pintype "bidirectional")
		)
		(pad "G15" smd circle
			(at 6.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "G16" smd circle
			(at 7.5 -1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 416 "FMC_D3")
			(pinfunction "IO_L36N_A8_M1BA1_1")
			(pintype "bidirectional")
		)
		(pad "H1" smd circle
			(at -7.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 389 "/fpga_ddr/DRAM_LDQSN")
			(pinfunction "IO_L39N_M3LDQSN_3")
			(pintype "bidirectional")
		)
		(pad "H2" smd circle
			(at -6.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 390 "/fpga_ddr/DRAM_LDQSP")
			(pinfunction "IO_L39P_M3LDQS_3")
			(pintype "bidirectional")
		)
		(pad "H3" smd circle
			(at -5.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/fpga_ddr/DRAM_ADDR6")
			(pinfunction "IO_L44N_GCLK20_M3A6_3")
			(pintype "bidirectional")
		)
		(pad "H4" smd circle
			(at -4.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "/fpga_ddr/DRAM_ADDR5")
			(pinfunction "IO_L44P_GCLK21_M3A5_3")
			(pintype "bidirectional")
		)
		(pad "H5" smd circle
			(at -3.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/fpga_ddr/DRAM_CASB")
			(pinfunction "IO_L43N_GCLK22_IRDY2_M3CASN_3")
			(pintype "bidirectional")
		)
		(pad "H6" smd circle
			(at -2.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "H7" smd circle
			(at -1.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "H8" smd circle
			(at -0.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "H9" smd circle
			(at 0.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "H10" smd circle
			(at 1.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "H11" smd circle
			(at 2.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 384 "unconnected-(U1B-IO_L38N_A4_M1CLKN_1-PadH11)")
			(pinfunction "IO_L38N_A4_M1CLKN_1")
			(pintype "bidirectional")
		)
		(pad "H12" smd circle
			(at 3.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "H13" smd circle
			(at 4.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 236 "DPI_R4")
			(pinfunction "IO_L39P_M1A3_1")
			(pintype "bidirectional")
		)
		(pad "H14" smd circle
			(at 5.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 237 "DPI_R3")
			(pinfunction "IO_L39N_M1ODT_1")
			(pintype "bidirectional")
		)
		(pad "H15" smd circle
			(at 6.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 421 "FMC_D4")
			(pinfunction "IO_L37P_A7_M1A0_1")
			(pintype "bidirectional")
		)
		(pad "H16" smd circle
			(at 7.5 -0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 408 "FMC_D5")
			(pinfunction "IO_L37N_A6_M1A1_1")
			(pintype "bidirectional")
		)
		(pad "J1" smd circle
			(at -7.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/fpga_ddr/DRAM_DATA3")
			(pinfunction "IO_L38N_M3DQ3_3")
			(pintype "bidirectional")
		)
		(pad "J2" smd circle
			(at -6.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VCCO_3")
			(pintype "power_in")
		)
		(pad "J3" smd circle
			(at -5.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/fpga_ddr/DRAM_DATA2")
			(pinfunction "IO_L38P_M3DQ2_3")
			(pintype "bidirectional")
		)
		(pad "J4" smd circle
			(at -4.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 397 "/fpga_ddr/DRAM_LDM")
			(pinfunction "IO_L42N_GCLK24_M3LDM_3")
			(pintype "bidirectional")
		)
		(pad "J5" smd circle
			(at -3.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "J6" smd circle
			(at -2.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/fpga_ddr/DRAM_RASB")
			(pinfunction "IO_L43P_GCLK23_M3RASN_3")
			(pintype "bidirectional")
		)
		(pad "J7" smd circle
			(at -1.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "J8" smd circle
			(at -0.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "J9" smd circle
			(at 0.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "J10" smd circle
			(at 1.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "J11" smd circle
			(at 2.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 357 "unconnected-(U1B-IO_L40P_GCLK11_M1A5_1-PadJ11)")
			(pinfunction "IO_L40P_GCLK11_M1A5_1")
			(pintype "bidirectional")
		)
		(pad "J12" smd circle
			(at 3.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 229 "DPI_G7")
			(pinfunction "IO_L40N_GCLK10_M1A6_1")
			(pintype "bidirectional")
		)
		(pad "J13" smd circle
			(at 4.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 226 "DPI_PCLK")
			(pinfunction "IO_L41P_GCLK9_IRDY1_M1RASN_1")
			(pintype "bidirectional")
		)
		(pad "J14" smd circle
			(at 5.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 238 "DPI_R2")
			(pinfunction "IO_L43P_GCLK5_M1DQ4_1")
			(pintype "bidirectional")
		)
		(pad "J15" smd circle
			(at 6.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_1")
			(pintype "power_in")
		)
		(pad "J16" smd circle
			(at 7.5 0.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 406 "FMC_D6")
			(pinfunction "IO_L43N_GCLK4_M1DQ5_1")
			(pintype "bidirectional")
		)
		(pad "K1" smd circle
			(at -7.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "/fpga_ddr/DRAM_DATA1")
			(pinfunction "IO_L37N_M3DQ1_3")
			(pintype "bidirectional")
		)
		(pad "K2" smd circle
			(at -6.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/fpga_ddr/DRAM_DATA0")
			(pinfunction "IO_L37P_M3DQ0_3")
			(pintype "bidirectional")
		)
		(pad "K3" smd circle
			(at -5.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 394 "/fpga_ddr/DRAM_UDM")
			(pinfunction "IO_L42P_GCLK25_TRDY2_M3UDM_3")
			(pintype "bidirectional")
		)
		(pad "K4" smd circle
			(at -4.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VCCO_3")
			(pintype "power_in")
		)
		(pad "K5" smd circle
			(at -3.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/fpga_ddr/DRAM_ADDR0")
			(pinfunction "IO_L47P_M3A0_3")
			(pintype "bidirectional")
		)
		(pad "K6" smd circle
			(at -2.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/fpga_ddr/DRAM_ADDR1")
			(pinfunction "IO_L47N_M3A1_3")
			(pintype "bidirectional")
		)
		(pad "K7" smd circle
			(at -1.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "K8" smd circle
			(at -0.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "K9" smd circle
			(at 0.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "K10" smd circle
			(at 1.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "+1V2_FPGA")
			(pinfunction "VCCINT")
			(pintype "power_in")
		)
		(pad "K11" smd circle
			(at 2.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 339 "GCLK")
			(pinfunction "IO_L42N_GCLK6_TRDY1_M1LDM_1")
			(pintype "bidirectional")
		)
		(pad "K12" smd circle
			(at 3.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 231 "DPI_G5")
			(pinfunction "IO_L42P_GCLK7_M1UDM_1")
			(pintype "bidirectional")
		)
		(pad "K13" smd circle
			(at 4.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_1")
			(pintype "power_in")
		)
		(pad "K14" smd circle
			(at 5.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 230 "DPI_G6")
			(pinfunction "IO_L41N_GCLK8_M1CASN_1")
			(pintype "bidirectional")
		)
		(pad "K15" smd circle
			(at 6.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 415 "FMC_D7")
			(pinfunction "IO_L44P_A3_M1DQ6_1")
			(pintype "bidirectional")
		)
		(pad "K16" smd circle
			(at 7.5 1.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 410 "FMC_NOE")
			(pinfunction "IO_L44N_A2_M1DQ7_1")
			(pintype "bidirectional")
		)
		(pad "L1" smd circle
			(at -7.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "/fpga_ddr/DRAM_DATA9")
			(pinfunction "IO_L36N_M3DQ9_3")
			(pintype "bidirectional")
		)
		(pad "L2" smd circle
			(at -6.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "L3" smd circle
			(at -5.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/fpga_ddr/DRAM_DATA8")
			(pinfunction "IO_L36P_M3DQ8_3")
			(pintype "bidirectional")
		)
		(pad "L4" smd circle
			(at -4.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/fpga_ddr/DRAM_ADDR3")
			(pinfunction "IO_L45P_M3A3_3")
			(pintype "bidirectional")
		)
		(pad "L5" smd circle
			(at -3.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "/fpga_ddr/DRAM_ODT")
			(pinfunction "IO_L45N_M3ODT_3")
			(pintype "bidirectional")
		)
		(pad "L6" smd circle
			(at -2.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "L7" smd circle
			(at -1.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 388 "unconnected-(U1C-IO_L62N_D6_2-PadL7)")
			(pinfunction "IO_L62N_D6_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "L8" smd circle
			(at -0.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 391 "unconnected-(U1C-IO_L62P_D5_2-PadL8)")
			(pinfunction "IO_L62P_D5_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "L9" smd circle
			(at 0.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "L10" smd circle
			(at 1.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 356 "FPGA_CS")
			(pinfunction "IO_L16P_2")
			(pintype "bidirectional")
		)
		(pad "L11" smd circle
			(at 2.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 393 "unconnected-(U1E-CMPCS_B_2-PadL11)")
			(pinfunction "CMPCS_B_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "L12" smd circle
			(at 3.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 228 "DPI_G2")
			(pinfunction "IO_L53P_1")
			(pintype "bidirectional")
		)
		(pad "L13" smd circle
			(at 4.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 227 "DPI_G3")
			(pinfunction "IO_L53N_VREF_1")
			(pintype "bidirectional")
		)
		(pad "L14" smd circle
			(at 5.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "DPI_G4")
			(pinfunction "IO_L47P_FWE_B_M1DQ0_1")
			(pintype "bidirectional")
		)
		(pad "L15" smd circle
			(at 6.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "L16" smd circle
			(at 7.5 2.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 405 "FMC_A16")
			(pinfunction "IO_L47N_LDC_M1DQ1_1")
			(pintype "bidirectional")
		)
		(pad "M1" smd circle
			(at -7.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/fpga_ddr/DRAM_DATA11")
			(pinfunction "IO_L35N_M3DQ11_3")
			(pintype "bidirectional")
		)
		(pad "M2" smd circle
			(at -6.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/fpga_ddr/DRAM_DATA10")
			(pinfunction "IO_L35P_M3DQ10_3")
			(pintype "bidirectional")
		)
		(pad "M3" smd circle
			(at -5.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+DRAM_VREF")
			(pinfunction "IO_L1N_VREF_3")
			(pintype "bidirectional")
		)
		(pad "M4" smd circle
			(at -4.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 334 "Net-(U1D-IO_L1P_3)")
			(pinfunction "IO_L1P_3")
			(pintype "bidirectional")
		)
		(pad "M5" smd circle
			(at -3.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 372 "unconnected-(U1D-IO_L2P_3-PadM5)")
			(pinfunction "IO_L2P_3")
			(pintype "bidirectional+no_connect")
		)
		(pad "M6" smd circle
			(at -2.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 387 "unconnected-(U1C-IO_L64P_D8_2-PadM6)")
			(pinfunction "IO_L64P_D8_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "M7" smd circle
			(at -1.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 349 "unconnected-(U1C-IO_L31N_GCLK30_D15_2-PadM7)")
			(pinfunction "IO_L31N_GCLK30_D15_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "M8" smd circle
			(at -0.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "M9" smd circle
			(at 0.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 339 "GCLK")
			(pinfunction "IO_L29P_GCLK3_2")
			(pintype "bidirectional")
		)
		(pad "M10" smd circle
			(at 1.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 348 "unconnected-(U1C-IO_L16N_VREF_2-PadM10)")
			(pinfunction "IO_L16N_VREF_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "M11" smd circle
			(at 2.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 199 "LVDS_EVEN_CN")
			(pinfunction "IO_L2N_CMPMOSI_2")
			(pintype "bidirectional")
		)
		(pad "M12" smd circle
			(at 3.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 198 "LVDS_EVEN_CP")
			(pinfunction "IO_L2P_CMPCLK_2")
			(pintype "bidirectional")
		)
		(pad "M13" smd circle
			(at 4.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 240 "DPI_B6")
			(pinfunction "IO_L74P_AWAKE_1")
			(pintype "bidirectional")
		)
		(pad "M14" smd circle
			(at 5.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 239 "DPI_B7")
			(pinfunction "IO_L74N_DOUT_BUSY_1")
			(pintype "bidirectional")
		)
		(pad "M15" smd circle
			(at 6.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 400 "FMC_D0")
			(pinfunction "IO_L46P_FCS_B_M1DQ2_1")
			(pintype "bidirectional")
		)
		(pad "M16" smd circle
			(at 7.5 3.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 354 "EPD_THROT")
			(pinfunction "IO_L46N_FOE_B_M1DQ3_1")
			(pintype "bidirectional")
		)
		(pad "N1" smd circle
			(at -7.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 376 "/fpga_ddr/DRAM_UDQSN")
			(pinfunction "IO_L34N_M3UDQSN_3")
			(pintype "bidirectional")
		)
		(pad "N2" smd circle
			(at -6.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 304 "+1V35")
			(pinfunction "VCCO_3")
			(pintype "power_in")
		)
		(pad "N3" smd circle
			(at -5.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 385 "/fpga_ddr/DRAM_UDQSP")
			(pinfunction "IO_L34P_M3UDQS_3")
			(pintype "bidirectional")
		)
		(pad "N4" smd circle
			(at -4.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 361 "unconnected-(U1D-IO_L2N_3-PadN4)")
			(pinfunction "IO_L2N_3")
			(pintype "bidirectional+no_connect")
		)
		(pad "N5" smd circle
			(at -3.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 382 "unconnected-(U1C-IO_L49P_D3_2-PadN5)")
			(pinfunction "IO_L49P_D3_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "N6" smd circle
			(at -2.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 392 "unconnected-(U1C-IO_L64N_D9_2-PadN6)")
			(pinfunction "IO_L64N_D9_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "N7" smd circle
			(at -1.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_2")
			(pintype "power_in")
		)
		(pad "N8" smd circle
			(at -0.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 288 "unconnected-(U1C-IO_L29N_GCLK2_2-PadN8)")
			(pinfunction "IO_L29N_GCLK2_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "N9" smd circle
			(at 0.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 398 "unconnected-(U1C-IO_L14P_D11_2-PadN9)")
			(pinfunction "IO_L14P_D11_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "N10" smd circle
			(at 1.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_2")
			(pintype "power_in")
		)
		(pad "N11" smd circle
			(at 2.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "IO_L13P_M1_2")
			(pintype "bidirectional")
		)
		(pad "N12" smd circle
			(at 3.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 378 "unconnected-(U1C-IO_L12P_D1_MISO2_2-PadN12)")
			(pinfunction "IO_L12P_D1_MISO2_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "N13" smd circle
			(at 4.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "N14" smd circle
			(at 5.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 242 "DPI_B4")
			(pinfunction "IO_L45P_A1_M1LDQS_1")
			(pintype "bidirectional")
		)
		(pad "N15" smd circle
			(at 6.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_1")
			(pintype "power_in")
		)
		(pad "N16" smd circle
			(at 7.5 4.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 417 "FMC_NWE")
			(pinfunction "IO_L45N_A0_M1LDQSN_1")
			(pintype "bidirectional")
		)
		(pad "P1" smd circle
			(at -7.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/fpga_ddr/DRAM_DATA13")
			(pinfunction "IO_L33N_M3DQ13_3")
			(pintype "bidirectional")
		)
		(pad "P2" smd circle
			(at -6.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/fpga_ddr/DRAM_DATA12")
			(pinfunction "IO_L33P_M3DQ12_3")
			(pintype "bidirectional")
		)
		(pad "P3" smd circle
			(at -5.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "P4" smd circle
			(at -4.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 210 "LVDS_ODD_AP")
			(pinfunction "IO_L63P_2")
			(pintype "bidirectional")
		)
		(pad "P5" smd circle
			(at -3.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 396 "unconnected-(U1C-IO_L49N_D4_2-PadP5)")
			(pinfunction "IO_L49N_D4_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "P6" smd circle
			(at -2.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 206 "LVDS_ODD_CP")
			(pinfunction "IO_L47P_2")
			(pintype "bidirectional")
		)
		(pad "P7" smd circle
			(at -1.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 351 "unconnected-(U1C-IO_L31P_GCLK31_D14_2-PadP7)")
			(pinfunction "IO_L31P_GCLK31_D14_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "P8" smd circle
			(at -0.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 202 "LVDS_EVEN_AP")
			(pinfunction "IO_L30P_GCLK1_D13_2")
			(pintype "bidirectional")
		)
		(pad "P9" smd circle
			(at 0.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 395 "unconnected-(U1C-IO_L14N_D12_2-PadP9)")
			(pinfunction "IO_L14N_D12_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "P10" smd circle
			(at 1.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 350 "FPGA_MOSI")
			(pinfunction "IO_L3P_D0_DIN_MISO_MISO1_2")
			(pintype "bidirectional")
		)
		(pad "P11" smd circle
			(at 2.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 380 "unconnected-(U1C-IO_L13N_D10_2-PadP11)")
			(pinfunction "IO_L13N_D10_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "P12" smd circle
			(at 3.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 377 "unconnected-(U1C-IO_L12N_D2_MISO3_2-PadP12)")
			(pinfunction "IO_L12N_D2_MISO3_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "P13" smd circle
			(at 4.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 333 "FPGA_DONE")
			(pinfunction "DONE_2")
			(pintype "bidirectional")
		)
		(pad "P14" smd circle
			(at 5.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 332 "FPGA_SUSP")
			(pinfunction "SUSPEND")
			(pintype "bidirectional")
		)
		(pad "P15" smd circle
			(at 6.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 241 "DPI_B5")
			(pinfunction "IO_L48P_HDC_M1DQ8_1")
			(pintype "bidirectional")
		)
		(pad "P16" smd circle
			(at 7.5 5.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 414 "FMC_NE1")
			(pinfunction "IO_L48N_M1DQ9_1")
			(pintype "bidirectional")
		)
		(pad "R1" smd circle
			(at -7.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "/fpga_ddr/DRAM_DATA15")
			(pinfunction "IO_L32N_M3DQ15_3")
			(pintype "bidirectional")
		)
		(pad "R2" smd circle
			(at -6.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/fpga_ddr/DRAM_DATA14")
			(pinfunction "IO_L32P_M3DQ14_3")
			(pintype "bidirectional")
		)
		(pad "R3" smd circle
			(at -5.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 363 "/fpga_config/FPGA_INIT")
			(pinfunction "IO_L65P_INIT_B_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "R4" smd circle
			(at -4.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_2")
			(pintype "power_in")
		)
		(pad "R5" smd circle
			(at -3.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 208 "LVDS_ODD_BP")
			(pinfunction "IO_L48P_D7_2")
			(pintype "bidirectional")
		)
		(pad "R6" smd circle
			(at -2.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "R7" smd circle
			(at -1.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 360 "LVDS_ODD_CKP")
			(pinfunction "IO_L32P_GCLK29_2")
			(pintype "bidirectional")
		)
		(pad "R8" smd circle
			(at -0.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_2")
			(pintype "power_in")
		)
		(pad "R9" smd circle
			(at 0.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 200 "LVDS_EVEN_BP")
			(pinfunction "IO_L23P_2")
			(pintype "bidirectional")
		)
		(pad "R10" smd circle
			(at 1.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "R11" smd circle
			(at 2.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 381 "FPGA_SCLK")
			(pinfunction "IO_L1P_CCLK_2")
			(pintype "bidirectional")
		)
		(pad "R12" smd circle
			(at 3.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 224 "DPI_HS")
			(pinfunction "IO_L52P_M1DQ14_1")
			(pintype "bidirectional")
		)
		(pad "R13" smd circle
			(at 4.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VCCO_1")
			(pintype "power_in")
		)
		(pad "R14" smd circle
			(at 5.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 243 "DPI_B3")
			(pinfunction "IO_L50P_M1UDQS_1")
			(pintype "bidirectional")
		)
		(pad "R15" smd circle
			(at 6.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 355 "unconnected-(U1B-IO_L49P_M1DQ10_1-PadR15)")
			(pinfunction "IO_L49P_M1DQ10_1")
			(pintype "bidirectional")
		)
		(pad "R16" smd circle
			(at 7.5 6.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 402 "FMC_D1")
			(pinfunction "IO_L49N_M1DQ11_1")
			(pintype "bidirectional")
		)
		(pad "T1" smd circle
			(at -7.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "T2" smd circle
			(at -6.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 331 "FPGA_PROG")
			(pinfunction "PROGRAM_B_2")
			(pintype "bidirectional")
		)
		(pad "T3" smd circle
			(at -5.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 386 "unconnected-(U1C-IO_L65N_CSO_B_2-PadT3)")
			(pinfunction "IO_L65N_CSO_B_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "T4" smd circle
			(at -4.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "LVDS_ODD_AN")
			(pinfunction "IO_L63N_2")
			(pintype "bidirectional")
		)
		(pad "T5" smd circle
			(at -3.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 209 "LVDS_ODD_BN")
			(pinfunction "IO_L48N_RDWR_B_VREF_2")
			(pintype "bidirectional")
		)
		(pad "T6" smd circle
			(at -2.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "LVDS_ODD_CN")
			(pinfunction "IO_L47N_2")
			(pintype "bidirectional")
		)
		(pad "T7" smd circle
			(at -1.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 358 "LVDS_ODD_CKN")
			(pinfunction "IO_L32N_GCLK28_2")
			(pintype "bidirectional")
		)
		(pad "T8" smd circle
			(at -0.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 203 "LVDS_EVEN_AN")
			(pinfunction "IO_L30N_GCLK0_USERCCLK_2")
			(pintype "bidirectional")
		)
		(pad "T9" smd circle
			(at 0.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 201 "LVDS_EVEN_BN")
			(pinfunction "IO_L23N_2")
			(pintype "bidirectional")
		)
		(pad "T10" smd circle
			(at 1.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 367 "FPGA_MISO")
			(pinfunction "IO_L3N_MOSI_CSI_B_MISO0_2")
			(pintype "bidirectional")
		)
		(pad "T11" smd circle
			(at 2.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "IO_L1N_M0_CMPMISO_2")
			(pintype "bidirectional")
		)
		(pad "T12" smd circle
			(at 3.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 225 "DPI_VS")
			(pinfunction "IO_L52N_M1DQ15_1")
			(pintype "bidirectional")
		)
		(pad "T13" smd circle
			(at 4.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 223 "DPI_DE")
			(pinfunction "IO_L51N_M1DQ13_1")
			(pintype "bidirectional")
		)
		(pad "T14" smd circle
			(at 5.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 244 "DPI_B2")
			(pinfunction "IO_L51P_M1DQ12_1")
			(pintype "bidirectional")
		)
		(pad "T15" smd circle
			(at 6.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 353 "unconnected-(U1B-IO_L50N_M1UDQSN_1-PadT15)")
			(pinfunction "IO_L50N_M1UDQSN_1")
			(pintype "bidirectional")
		)
		(pad "T16" smd circle
			(at 7.5 7.5 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_BGA.3dshapes/Xilinx_FTG256.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.47 87.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at -2.59 0.87 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R/1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25105"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "DPI_PCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 251 "/tmds_in/ADV_CK")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 114.45 66.95 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C103"
			(at 3.15 -0.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 115.6 37.5125 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB3"
			(at -2.7125 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100M"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14709"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 374 "+3V3A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC"
		(layer "F.Cu")
		(at 151 74 -90)
		(descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
		(tags "SMD SMT SPST EVQPUL EVQPUC")
		(property "Reference" "SW1"
			(at 0 3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SW"
			(at 0 3.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C79174"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.375 90)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0 1.375 90)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "1" smd rect
			(at -2.625 -0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 347 "KEY1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 2.625 -0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 347 "KEY1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.625 0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.625 0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/EVQPU-LC-02K.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 74.1 59 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D8"
			(at 0 -1.43 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED GREEN"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C965804"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "fpga_io")
		(sheetfile "fpga_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 129.3 58.2 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -2.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 135.7 64.9 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R124"
			(at -0.69 3.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 309 "Net-(U13-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 135.795 78.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C115"
			(at -2.395 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 118.675 105.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 1.8 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 127 102.2)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 456 "Net-(U10-SET)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:modos_logo"
		(layer "F.Cu")
		(at 138.6 49.6)
		(property "Reference" "G***"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "footprints:modos_logo"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 82.05 37.7 180)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L6"
			(at 2.4 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 458 "Net-(D3-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
		(layer "F.Cu")
		(at 135.8 81.8)
		(descr "http://www.onsemi.com/pub/Collateral/510CD.PDF")
		(tags "WQFN-20 4.5mm 2.5mm 0.5mm")
		(property "Reference" "U18"
			(at -3.4 0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CBTL02043A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/CBTL02043A_CBTL02043B.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2652457"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WQFN*1EP*2.5x4.5mm*P0.5mm*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at 0 -0.95 270)
			(size 0.8 0.8)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at 0 0.95 270)
			(size 0.8 0.8)
			(layers "F.Paste")
		)
		(pad "1" smd rect
			(at -0.25 -2.3 270)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.3 -1.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "XSD")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.3 -1.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 179 "/dp_in/DP1N")
			(pinfunction "A0_P")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 -0.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 180 "/dp_in/DP1P")
			(pinfunction "A0_N")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.3 -0.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at -1.3 0.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.3 0.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 181 "/dp_in/DP0N")
			(pinfunction "A1_P")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -1.3 1.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 182 "/dp_in/DP0P")
			(pinfunction "A1_N")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.3 1.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 177 "TYPEC_ORI")
			(pinfunction "SEL")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -0.25 2.3 270)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.25 2.3 270)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.3 1.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "/dp_in/RX1PC")
			(pinfunction "C1_N")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 1.3 1.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "/dp_in/RX1NC")
			(pinfunction "C1_P")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.3 0.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "/dp_in/TX1PC")
			(pinfunction "C0_N")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.3 0.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "/dp_in/TX1NC")
			(pinfunction "C0_P")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 1.3 -0.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "/dp_in/RX2PC")
			(pinfunction "B1_N")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 1.3 -0.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "/dp_in/RX2NC")
			(pinfunction "B1_P")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 1.3 -1.25)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 149 "/dp_in/TX2PC")
			(pinfunction "B0_N")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 1.3 -1.75)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "/dp_in/TX2NC")
			(pinfunction "B0_P")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 0.25 -2.3 270)
			(size 0.9 0.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 0 0 270)
			(size 2.9 1)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 82.85 46)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 1.6 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 303 "+5V_EG")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 132.2 42.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 87.45 43.2)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U24"
			(at -2.6 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LGS6302B5"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304071430_Legend-Si-LGS6302_C5123975.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.5A, 1.2MHz Boost DC/DC Converter, adjustable 3-60V output voltage, SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5123975"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "Net-(D2-A)")
			(pinfunction "SW")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U24-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 453 "/epd_power/+5V_VGH")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 453 "/epd_power/+5V_VGH")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 80.95 49.6)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at -3.15 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 79.7 55.7 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(U6-SET)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 82.91 104.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C71"
			(at 0 -1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102 86.7 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C66"
			(at -0.1 2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 285 "+1V2_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U28-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(at 145.5 58)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H1"
			(at 0 -2.9 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 2.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "DNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 125.5 80.5 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -2.5 0.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "DP_PDN")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 111.4 84.85 90)
		(property "Reference" "H16"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.01 0.04 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 107.8 86.6 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at -2.7 1.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 117.9 38.1 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 1.9 -0.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 374 "+3V3A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 84.8 57.15 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C104"
			(at 0 -1.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 126.7 80.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C123"
			(at 2.5 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at -9.975841 -15.655672 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "Net-(C117-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-6"
		(layer "F.Cu")
		(at 98.85 43.2)
		(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U26"
			(at 2.05 4.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LGS5145"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5123971"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT*23*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(U26-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(U26-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 330 "/epd_power/EN_VN")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "+5V_ES")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 459 "Net-(D17-K)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 82.05 34.8 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 2.2 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 96 35.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C166"
			(at -2.6 -0.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 73.775 86.75 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C158"
			(at 7.65 -0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 105 99.4)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L8"
			(at 2.6 -1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "Net-(U2-SW)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 300 "+1V35_DCDC")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 118.15 67.35 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -53 111.830748 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "Net-(U4-SET)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 103.6 37.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 3 0.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25768"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U11-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 294 "VCOM_DAC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.19 46.85 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -0.01 -3.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 128.22 87.5 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN8"
			(at 1.5 -0.22 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 255 "/tmds_in/ADV_P8")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "/tmds_in/ADV_P9")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 257 "/tmds_in/ADV_P10")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 256 "/tmds_in/ADV_P11")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 227 "DPI_G3")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 228 "DPI_G2")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 342 "unconnected-(RN8-R2.2-Pad7)")
			(pinfunction "R2.2")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 341 "unconnected-(RN8-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 110.1 36.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C163"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 337 "VP_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.6 86.6 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C151"
			(at 0 1.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.2 44.3 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R62"
			(at 0 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "Net-(Q6-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(layer "F.Cu")
		(at 142.8 85.2375 180)
		(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
		(tags "UDFN-10 U-DFN2510-10 Diodes")
		(property "Reference" "D11"
			(at -1.6 0.0375 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RCLAMP0524P"
			(at 0 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C907837"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "UDFN*1.0x3.8mm*P0.5mm*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/dp_in/RX1P")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/dp_in/RX1N")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.35 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "/dp_in/TX1P")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/dp_in/TX1N")
			(pinfunction "IO4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/dp_in/TX1N")
			(pinfunction "NC1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "/dp_in/TX1P")
			(pinfunction "NC2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.4125 0 90)
			(size 0.45 0.575)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/dp_in/RX1N")
			(pinfunction "NC3")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/dp_in/RX1P")
			(pinfunction "NC4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 111.4 103.4 90)
		(property "Reference" "H20"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.02 0.11 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.7 51.8)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C164"
			(at 1.4 -0.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "VGH_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 98.9 40.4 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D17"
			(at 2.8 2.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 459 "Net-(D17-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 143.8 105.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C170"
			(at -1.6 -0.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14442"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 222 "/tmds_in/HDMI_HPD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.2 55.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R92"
			(at 8.8 1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 330 "/epd_power/EN_VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "Net-(D1-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 129.2 103.8 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C161"
			(at 2.8 0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 96.85 46.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R88"
			(at -2.1 -0.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "390K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25782"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(U26-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 132.7 66 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C101"
			(at 2.2 0.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 313 "Net-(U13-BST1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 314 "Net-(U13-SW1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 126.6 69.62 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C118"
			(at 0.12 1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "Net-(C118-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 127.05 38.45)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at -0.05 -4.65 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 368 "/mcu/OSC32_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 87.45 39.6 180)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L5"
			(at 2.4 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 453 "/epd_power/+5V_VGH")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "Net-(D2-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 87.2 50.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C178"
			(at 3.1 2.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 303 "+5V_EG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 87 63.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_io")
		(sheetfile "fpga_io.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "/fpga_io/LED")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "Net-(D8-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 117.525 88.9)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 4.275 -0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "240K/1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C64043"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 307 "+1V8_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "Net-(U20-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 101.5 58.25)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D4"
			(at -2.4 1.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0.35 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:8P_2.54"
		(layer "F.Cu")
		(at 68.4 47 -90)
		(property "Reference" "J2"
			(at -10.4 1.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08_MountingPin"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:8P_2.54"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "DNP"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "user_ext")
		(sheetfile "user_extension.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -8.89 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -6.35 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 447 "USER_PD8")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -3.81 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 450 "USER_PD9")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -1.27 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 446 "USER_PD10")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 1.27 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 448 "USER_PD13")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 3.81 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 449 "USER_PB8")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 6.35 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 445 "USER_PB9")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 8.89 0 270)
			(size 1.27 5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 107.7 83.3 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C67"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 285 "+1V2_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.2 56.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R93"
			(at 8.8 1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "/epd_power/EN_VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "Net-(D4-K)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 145.4 92.442305 90)
		(property "Reference" "H22"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.03 0.01 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 101.7 35.8 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C177"
			(at 2.6 2.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 80.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C109"
			(at -4.8 -0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "/dp_in/RX2N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "/dp_in/RX2NC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:USB_C_Receptacle_GT-USB-7007A"
		(layer "F.Cu")
		(at 153.3625 84.89925 90)
		(property "Reference" "J1"
			(at -3.70075 -6.3625 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "GT-USB-7007A"
			(at 0 -7.62 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:USB_C_Receptacle_GT-USB-7007A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5299422"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0375 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd rect
			(at -2.625 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "A2" smd rect
			(at -2.125 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/dp_in/RX1P")
			(pinfunction "TX1+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A3" smd rect
			(at -1.625 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/dp_in/RX1N")
			(pinfunction "TX1-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A4" smd rect
			(at -1.125 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "+VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "A5" smd rect
			(at -0.625 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "/dp_in/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A6" smd rect
			(at -0.125 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 319 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A7" smd rect
			(at 0.375 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 320 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A8" smd rect
			(at 0.875 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "/dp_in/SBU1")
			(pinfunction "SBU1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A9" smd rect
			(at 1.375 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "+VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "A10" smd rect
			(at 1.875 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "/dp_in/TX2N")
			(pinfunction "RX2-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A11" smd rect
			(at 2.375 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "/dp_in/TX2P")
			(pinfunction "RX2+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A12" smd rect
			(at 2.875 -5.525 90)
			(size 0.27 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "B1" smd rect
			(at 2.62 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "B2" smd rect
			(at 2.12 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "/dp_in/RX2P")
			(pinfunction "TX2+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B3" smd rect
			(at 1.62 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "/dp_in/RX2N")
			(pinfunction "TX2-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B4" smd rect
			(at 1.12 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "+VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "B5" smd rect
			(at 0.62 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "/dp_in/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B6" smd rect
			(at 0.12 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 319 "Net-(J1-D+-PadA6)")
			(pinfunction "D+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B7" smd rect
			(at -0.38 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 320 "Net-(J1-D--PadA7)")
			(pinfunction "D-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B8" smd rect
			(at -0.88 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "/dp_in/SBU2")
			(pinfunction "SBU2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B9" smd rect
			(at -1.38 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "+VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "B10" smd rect
			(at -1.88 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/dp_in/TX1N")
			(pinfunction "RX1-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B11" smd rect
			(at -2.38 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "/dp_in/TX1P")
			(pinfunction "RX1+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B12" smd rect
			(at -2.88 -4.125 90)
			(size 0.27 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S1" thru_hole oval
			(at -5.52 0 90)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S1" thru_hole oval
			(at -4.325 -4.85 90)
			(size 1 2)
			(drill oval 0.6 1.6)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4 -4.35 90)
			(size 1.54 1)
			(drill oval 1.2 0.6)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4 -4.35 90)
			(size 1.54 1)
			(drill oval 1.2 0.6)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.325 -4.85 90)
			(size 1 2)
			(drill oval 0.6 1.6)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 5.52 0 90)
			(size 1 1.6)
			(drill oval 0.6 1.2)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/USB-C-SMD_TYPE-C-GT-USB-7007C.step"
			(offset
				(xyz -0.12 4.2 -0.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 104.9375 41.6)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U11"
			(at 0.1625 5.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LM321"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm321.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C9405"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U11-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(Q6-S)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(Q6-S)")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 57.4)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R117"
			(at 9.065 2.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "VGL_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 130.25025 75.89975 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -0.14975 1.09975 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "Net-(U19-TESTMODE)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 87.45 34.8)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 2.15 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "+VGH")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 120.8 66.95)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U4"
			(at 0 -2.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MT9700"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C89855"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "Net-(U4-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 78.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C107"
			(at -1.8 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 120 "/dp_in/TX2N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "/dp_in/TX2NC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(layer "F.Cu")
		(at 141.6075 94.4 180)
		(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
		(tags "UDFN-10 U-DFN2510-10 Diodes")
		(property "Reference" "D9"
			(at -1.5625 -0.149998 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RCLAMP0524P"
			(at 0 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C907837"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "UDFN*1.0x3.8mm*P0.5mm*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "/tmds_in/TMDS_D1N")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 183 "/tmds_in/TMDS_D1P")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.35 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "/tmds_in/TMDS_D2N")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 214 "/tmds_in/TMDS_D2P")
			(pinfunction "IO4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 214 "/tmds_in/TMDS_D2P")
			(pinfunction "NC1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "/tmds_in/TMDS_D2N")
			(pinfunction "NC2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.4125 0 90)
			(size 0.45 0.575)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 183 "/tmds_in/TMDS_D1P")
			(pinfunction "NC3")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "/tmds_in/TMDS_D1N")
			(pinfunction "NC4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 120.3 83.2 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 307 "+1V8_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 101.5375 49.95)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 2.6625 0.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "S8050"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C444723"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "Net-(Q1-G)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1206_3216Metric"
		(layer "F.Cu")
		(at 139.7 75 180)
		(descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -3.5 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "3A"
			(at 0 1.82 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Fuse:Fuse_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14165"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 324 "+VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 310 "Net-(U13-VIN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 145.3 50.97 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D19"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED GREEN"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C965804"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 323 "Net-(D19-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 130.72 87.5 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN9"
			(at 1.5 -0.52 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 262 "/tmds_in/ADV_P12")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 259 "/tmds_in/ADV_P13")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 260 "/tmds_in/ADV_P14")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 261 "/tmds_in/ADV_P15")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 229 "DPI_G7")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 230 "DPI_G6")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 231 "DPI_G5")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "DPI_G4")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.9375 51.35 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -0.97 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(Q2-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 123.6 80.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C119"
			(at 2.3 -0.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at -9.975841 -15.655672 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 90.735 49.15)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at -0.035 1.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 302 "+5V_ES")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
		(layer "F.Cu")
		(at 124.3 75.3 90)
		(descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U19"
			(at 4.7 -4.9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PTN3460"
			(at 0 4.82 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PTN3460.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C5190369"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -2.1 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -2.1 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -2.1 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -2.1 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -0.7 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -0.7 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -0.7 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -0.7 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 0.7 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 0.7 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 0.7 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 0.7 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 2.1 -2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 2.1 -0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 2.1 0.7 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 2.1 2.1 90)
			(size 1.13 1.13)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "/dp_in/DPAUXN")
			(pinfunction "AUX_N")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 163 "/dp_in/DPAUXP")
			(pinfunction "AUX_P")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "/dp_in/DP0P")
			(pinfunction "DP0_P")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -3.4375 -1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "/dp_in/DP0N")
			(pinfunction "DP0_N")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "VDD18")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -3.4375 -0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 180 "/dp_in/DP1P")
			(pinfunction "DP1_P")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -3.4375 0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 179 "/dp_in/DP1N")
			(pinfunction "DP1_N")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -3.4375 0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 249 "DEC_RST")
			(pinfunction "RST_N")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -3.4375 1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "DP_PDN")
			(pinfunction "PD_N")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -3.4375 1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "DP_HPD")
			(pinfunction "HPDRX")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -3.4375 1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "unconnected-(U19-DEV_CFG-Pad12)")
			(pinfunction "DEV_CFG")
			(pintype "input+no_connect")
		)
		(pad "13" smd roundrect
			(at -3.4375 2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "Net-(C117-Pad1)")
			(pinfunction "VDD33")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at -3.4375 2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "Net-(C117-Pad1)")
			(pinfunction "VDD33")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at -2.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "unconnected-(U19-NC-Pad15)")
			(pinfunction "NC")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at -2.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 186 "unconnected-(U19-NC-Pad16)")
			(pinfunction "NC")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at -1.8 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GNDREG")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at -1.4 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GNDREG")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -1 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 282 "unconnected-(U19-VDD18REG-Pad19)")
			(pinfunction "VDD18REG")
			(pintype "power_out+no_connect")
		)
		(pad "20" smd roundrect
			(at -0.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "Net-(U19-TESTMODE)")
			(pinfunction "TESTMODE")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -0.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 187 "unconnected-(U19-CFG1-Pad21)")
			(pinfunction "CFG1")
			(pintype "input+no_connect")
		)
		(pad "22" smd roundrect
			(at 0.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 188 "unconnected-(U19-CFG2-Pad22)")
			(pinfunction "CFG2")
			(pintype "input+no_connect")
		)
		(pad "23" smd roundrect
			(at 0.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "unconnected-(U19-CFG3-Pad23)")
			(pinfunction "CFG3")
			(pintype "input+no_connect")
		)
		(pad "24" smd roundrect
			(at 1 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "MS_SDA")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 1.4 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "MS_SCL")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 1.8 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "LVDS_BKLTEN")
			(pinfunction "BKLTEN")
			(pintype "output")
		)
		(pad "27" smd roundrect
			(at 2.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 191 "unconnected-(U19-CFG4-Pad27)")
			(pinfunction "CFG4")
			(pintype "input+no_connect")
		)
		(pad "28" smd roundrect
			(at 2.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "unconnected-(U19-PWMO-Pad28)")
			(pinfunction "PWMO")
			(pintype "output+no_connect")
		)
		(pad "29" smd roundrect
			(at 3.4375 2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "unconnected-(U19-DDC_SCL-Pad29)")
			(pinfunction "DDC_SCL")
			(pintype "open_collector+no_connect")
		)
		(pad "30" smd roundrect
			(at 3.4375 2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 194 "unconnected-(U19-DDC_SDA-Pad30)")
			(pinfunction "DDC_SDA")
			(pintype "open_collector+no_connect")
		)
		(pad "31" smd roundrect
			(at 3.4375 1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 195 "unconnected-(U19-LVSDE_N-Pad31)")
			(pinfunction "LVSDE_N")
			(pintype "output+no_connect")
		)
		(pad "32" smd roundrect
			(at 3.4375 1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 196 "unconnected-(U19-LVSDE_P-Pad32)")
			(pinfunction "LVSDE_P")
			(pintype "output+no_connect")
		)
		(pad "33" smd roundrect
			(at 3.4375 1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 317 "LVDS_PVCCEN")
			(pinfunction "PVCCEN")
			(pintype "output")
		)
		(pad "34" smd roundrect
			(at 3.4375 0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 362 "unconnected-(U19-LVSCKE_P-Pad34)")
			(pinfunction "LVSCKE_P")
			(pintype "output+no_connect")
		)
		(pad "35" smd roundrect
			(at 3.4375 0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 359 "unconnected-(U19-LVSCKE_N-Pad35)")
			(pinfunction "LVSCKE_N")
			(pintype "output+no_connect")
		)
		(pad "36" smd roundrect
			(at 3.4375 -0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 198 "LVDS_EVEN_CP")
			(pinfunction "LVSCE_P")
			(pintype "output")
		)
		(pad "37" smd roundrect
			(at 3.4375 -0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "LVDS_EVEN_CN")
			(pinfunction "LVSCE_N")
			(pintype "output")
		)
		(pad "38" smd roundrect
			(at 3.4375 -1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "Net-(C118-Pad1)")
			(pinfunction "VDD33")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at 3.4375 -1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 200 "LVDS_EVEN_BP")
			(pinfunction "LVSBE_P")
			(pintype "output")
		)
		(pad "40" smd roundrect
			(at 3.4375 -1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "LVDS_EVEN_BN")
			(pinfunction "LVSBE_N")
			(pintype "output")
		)
		(pad "41" smd roundrect
			(at 3.4375 -2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 202 "LVDS_EVEN_AP")
			(pinfunction "LVSAE_P")
			(pintype "output")
		)
		(pad "42" smd roundrect
			(at 3.4375 -2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 203 "LVDS_EVEN_AN")
			(pinfunction "LVSAE_N")
			(pintype "output")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 204 "unconnected-(U19-LVSDO_P-Pad43)")
			(pinfunction "LVSDO_P")
			(pintype "output+no_connect")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 205 "unconnected-(U19-LVSDO_N-Pad44)")
			(pinfunction "LVSDO_N")
			(pintype "output+no_connect")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pinfunction "VDD18")
			(pintype "power_in")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 360 "LVDS_ODD_CKP")
			(pinfunction "LVSCKO_P")
			(pintype "output")
		)
		(pad "47" smd roundrect
			(at 1 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 358 "LVDS_ODD_CKN")
			(pinfunction "LVSCKO_N")
			(pintype "output")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 206 "LVDS_ODD_CP")
			(pinfunction "LVSCO_P")
			(pintype "output")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 207 "LVDS_ODD_CN")
			(pinfunction "LVSCO_N")
			(pintype "output")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "Net-(C118-Pad1)")
			(pinfunction "VDD33")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 208 "LVDS_ODD_BP")
			(pinfunction "LVSBO_P")
			(pintype "output")
		)
		(pad "52" smd roundrect
			(at -1 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 209 "LVDS_ODD_BN")
			(pinfunction "LVSBO_N")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 210 "LVDS_ODD_AP")
			(pinfunction "LVSAO_P")
			(pintype "output")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 211 "LVDS_ODD_AN")
			(pinfunction "LVSAO_N")
			(pintype "output")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "unconnected-(U19-NC-Pad55)")
			(pinfunction "NC")
			(pintype "input")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "EPS_N")
			(pintype "input")
		)
		(pad "57" smd rect
			(at 0 0 90)
			(size 5.6 5.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "EP")
			(pintype "input")
			(zone_connect 2)
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.2 54.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 8.8 1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 330 "/epd_power/EN_VN")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 80.4 103.2 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C148"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 135.4 76.7)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C99"
			(at -2.8 -0.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 310 "Net-(U13-VIN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 111.7 54.72 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -4.08 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 130.15 78.425 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB1"
			(at 0.000001 1.300001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120R@100M"
			(at 0 1.43 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C14709"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "Net-(C117-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.2 52.4 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 -3.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0006"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 333 "FPGA_DONE")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.2 58.2 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -2.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 114.025 40.375 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 1.975 -0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.2 53.4 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 -3.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0006"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 331 "FPGA_PROG")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 123.05 36.025 180)
		(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at 0 3.225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "24MHz"
			(at 0 2.45 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C70590"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0.85 180)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 365 "/mcu/OSC_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0.85 180)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.1 -0.85 180)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 366 "Net-(C10-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.1 -0.85 180)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 84.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C105"
			(at -4.8 -0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "/dp_in/RX1N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "/dp_in/RX1NC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102 88.6 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R58"
			(at 0 2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U28-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 101.1 102.4 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "150K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25755"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 300 "+1V35_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "Net-(U2-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.2 51.4)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 3.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0006"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 332 "FPGA_SUSP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 117.425 96.2875)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -2.4 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(layer "F.Cu")
		(at 141.6075 97.6 180)
		(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
		(tags "UDFN-10 U-DFN2510-10 Diodes")
		(property "Reference" "D10"
			(at -1.5625 0.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RCLAMP0524P"
			(at 0 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C907837"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "UDFN*1.0x3.8mm*P0.5mm*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "/tmds_in/TMDS_CKN")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "/tmds_in/TMDS_CKP")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.35 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "/tmds_in/TMDS_D0N")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "/tmds_in/TMDS_D0P")
			(pinfunction "IO4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "/tmds_in/TMDS_D0P")
			(pinfunction "NC1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "/tmds_in/TMDS_D0N")
			(pinfunction "NC2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.4125 0 90)
			(size 0.45 0.575)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "/tmds_in/TMDS_CKP")
			(pinfunction "NC3")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "/tmds_in/TMDS_CKN")
			(pinfunction "NC4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 91.25 47.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R79"
			(at -1.05 -3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "13K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25754"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "Net-(U23-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.7 80.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C117"
			(at 2.5 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "Net-(C117-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 125 102.2 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 455 "HPD_EN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.32 102.8)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C139"
			(at 0 4.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.5 37.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0.1 1.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 84.55 53.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 5.75 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 118.42 75.9 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C124"
			(at -0.03 0.975 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "Net-(C118-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 109.0125 45.15 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q7"
			(at 0 -3.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AO3401A"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C347476"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "Net-(Q7-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "Net-(Q6-G)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91.4 104.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C75"
			(at 0 -1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 103.6 72.35 180)
		(descr "Miniature Crystal Clock Oscillator Abracon ASE series, http://www.abracon.com/Oscillators/ASEseries.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal oscillator")
		(property "Reference" "X1"
			(at 0 -2.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33.33MHz"
			(at 0 2.45 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.abracon.com/Oscillators/ASV.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C46598403"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Oscillator*SMD*Abracon*ASE*3.2x2.5mm*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 0.825 180)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.05 0.825 180)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 1.05 -0.825 180)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "Net-(X1-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -1.05 -0.825 180)
			(size 1.3 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "Vdd")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASE-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 124.62 92.5 180)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN12"
			(at 1.700001 -0.050001 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 273 "/tmds_in/ADV_P4")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 274 "/tmds_in/ADV_P5")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 271 "/tmds_in/ADV_P6")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 272 "/tmds_in/ADV_P7")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 239 "DPI_B7")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 240 "DPI_B6")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 241 "DPI_B5")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 242 "DPI_B4")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.1 104.4 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 2.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "120K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25750"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "Net-(U2-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 142.6 51)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 1.07 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 335 "/mcu/G_LED")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 323 "Net-(D19-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 108 39.15 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R64"
			(at 0 3.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25768"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 157 "Net-(Q8-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 284 "-VCOM")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.85 45.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C175"
			(at 0 -0.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(U26-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 102.2 40.31 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U11-+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.6 83.8 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C65"
			(at -2.1 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U28-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U28-BS)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(layer "F.Cu")
		(at 142.8275 88.3625)
		(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
		(tags "UDFN-10 U-DFN2510-10 Diodes")
		(property "Reference" "D13"
			(at 1.5725 0.0375 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RCLAMP0524P"
			(at 0 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C907837"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "UDFN*1.0x3.8mm*P0.5mm*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.3875 -1 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "/dp_in/SBU2")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.3875 -0.5 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "/dp_in/SBU1")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.35 0 270)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.3875 0.5 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "/dp_in/CC1")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.3875 1 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "/dp_in/CC2")
			(pinfunction "IO4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.3875 1 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "/dp_in/CC2")
			(pinfunction "NC1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.3875 0.5 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "/dp_in/CC1")
			(pinfunction "NC2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.4125 0 270)
			(size 0.45 0.575)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.3875 -0.5 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "/dp_in/SBU1")
			(pinfunction "NC3")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.3875 -1 270)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "/dp_in/SBU2")
			(pinfunction "NC4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.6 100.2 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -1.6 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "Net-(U2-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U2-BS)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 109.95 84.85 90)
		(property "Reference" "H13"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.01 0.04 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 87.335 53.15 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R54"
			(at -5.45 -0.035 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 303 "+5V_EG")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm"
		(layer "F.Cu")
		(at 141.3 103.3 -90)
		(descr "WQFN, 14 Pin (https://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF#page=32), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "WQFN NoLead")
		(property "Reference" "U17"
			(at -0.000002 -2.55 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FUSB302BMPX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C132291"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WQFN*2.5x2.5mm*P0.5mm*EP1.45x1.45mm*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.36 -0.36 270)
			(size 0.58 0.58)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.36 0.36 270)
			(size 0.58 0.58)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.36 -0.36 270)
			(size 0.58 0.58)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.36 0.36 270)
			(size 0.58 0.58)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.2625 -0.5 270)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 171 "/dp_in/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.2625 0 270)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 324 "+VBUS")
			(pinfunction "VBUS")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.2625 0.5 270)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -0.75 1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -0.25 1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "TCPC_INT")
			(pinfunction "INT_N")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at 0.25 1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 0.75 1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 1.2625 0.5 270)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 1.2625 0 270)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 1.2625 -0.5 270)
			(size 0.675 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 168 "/dp_in/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 0.75 -1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 168 "/dp_in/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 0.25 -1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VCONN")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at -0.25 -1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VCONN")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at -0.75 -1.2625 270)
			(size 0.25 0.675)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 171 "/dp_in/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 0 0 270)
			(size 1.45 1.45)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TDFN-6-1EP_2.5x2.5mm_P0.65mm_EP1.3x2mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 124.62 90.75 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C127"
			(at -0.5 1.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 84.5 93.1 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C80"
			(at 0 1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.3 92.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C77"
			(at 2.1 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.7 49.8 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R98"
			(at 1.99 0.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "VGH_MEA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "+VGH")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOT-666-Alt"
		(layer "F.Cu")
		(at 142.4 82.5 180)
		(descr "SOT666")
		(tags "SOT-666")
		(property "Reference" "U16"
			(at -2 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USBLC6-2P6"
			(at 0 1.75 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:SOT-666-Alt"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C15999"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?666*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.75 -0.5375 180)
			(size 0.7 0.375)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 319 "Net-(J1-D+-PadA6)")
			(pinfunction "I/O1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.825 0 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -0.75 0.5375 180)
			(size 0.7 0.375)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 320 "Net-(J1-D--PadA7)")
			(pinfunction "I/O2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.75 0.5375 180)
			(size 0.7 0.375)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "USB_DN")
			(pinfunction "I/O2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 0.825 0 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 324 "+VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 0.75 -0.5375 180)
			(size 0.7 0.375)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 169 "USB_DP")
			(pinfunction "I/O1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-666.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 92 61.5)
		(property "Reference" "H25"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.01 0.15 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 79.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C108"
			(at -4.8 -0.3 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 148 "/dp_in/TX2P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 149 "/dp_in/TX2PC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 85.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C106"
			(at -4.8 -0.35 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/dp_in/RX1P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "/dp_in/RX1PC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91.25 45.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C165"
			(at 1.25 4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "Net-(U23-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.2 45.75 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -0.01 -3.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 84.55 51.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 6.75 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 76.1 46.65 90)
		(property "Reference" "H6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.03 0.04 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.09 39.15 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R65"
			(at -1.91 -0.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "VCOM_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 124.62 97.75 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C131"
			(at 2.5 -0.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-100_14x14mm_P0.5mm"
		(layer "F.Cu")
		(at 122.2 48.275 -90)
		(descr "LQFP, 100 Pin (https://www.nxp.com/docs/en/package-information/SOT407-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U3"
			(at -7.675 -8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "STM32H750VBTx"
			(at 0 9.42 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h750vb.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M7 MCU, 128KB flash, 1024KB RAM, 480 MHz, 1.71-3.6V, 82 GPIO, LQFP100"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C404010"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LQFP*14x14mm*P0.5mm*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.675 -6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 419 "QSPI_SD2")
			(pinfunction "PE2")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -7.675 -5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 143 "KEY3")
			(pinfunction "PE3")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -7.675 -5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 347 "KEY1")
			(pinfunction "PE4")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -7.675 -4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "LVDS_BKLTEN")
			(pinfunction "PE5")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -7.675 -4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 317 "LVDS_PVCCEN")
			(pinfunction "PE6")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -7.675 -3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VBAT")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -7.675 -3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 411 "unconnected-(U3-PC13-Pad7)")
			(pinfunction "PC13")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -7.675 -2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 368 "/mcu/OSC32_IN")
			(pinfunction "PC14")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -7.675 -2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 369 "/mcu/OSC32_OUT")
			(pinfunction "PC15")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -7.675 -1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -7.675 -1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -7.675 -0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 365 "/mcu/OSC_IN")
			(pinfunction "PH0")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -7.675 0 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 379 "/mcu/OSC_OUT")
			(pinfunction "PH1")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -7.675 0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 371 "Net-(U3-NRST)")
			(pinfunction "NRST")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -7.675 1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 413 "unconnected-(U3-PC0-Pad15)")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -7.675 1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 139 "SDIO_CLK")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -7.675 2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 367 "FPGA_MISO")
			(pinfunction "PC2_C")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -7.675 2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 350 "FPGA_MOSI")
			(pinfunction "PC3_C")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -7.675 3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VSSA")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at -7.675 3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 374 "+3V3A")
			(pinfunction "VREF+")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -7.675 4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 374 "+3V3A")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "22" smd roundrect
			(at -7.675 4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "SDIO_CMD")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at -7.675 5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 409 "QSPI_SD3")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at -7.675 5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 159 "VCOM_MEA_EN")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at -7.675 6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 158 "VCOM_EN")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at -6 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at -5.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at -5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 294 "VCOM_DAC")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -4.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 329 "VGH_DAC")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -4 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 337 "VP_MEA")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at -3.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "VCOM_MEA")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at -3 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "VGH_MEA")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at -2.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 340 "VN_MEA")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -2 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "VGL_MEA")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at -1.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "VBUS_MEA")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at -1 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 316 "QSPI_SCLK")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at -0.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 421 "FMC_D4")
			(pinfunction "PE7")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 0 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 408 "FMC_D5")
			(pinfunction "PE8")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 0.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 406 "FMC_D6")
			(pinfunction "PE9")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 1 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 415 "FMC_D7")
			(pinfunction "PE10")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 1.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 454 "Net-(U3-PE11)")
			(pinfunction "PE11")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 2 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 221 "EPD_POS_EN")
			(pinfunction "PE12")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at 2.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "FL_PWM1")
			(pinfunction "PE13")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 3 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "FL_PWM2")
			(pinfunction "PE14")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 3.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 326 "FL_EN")
			(pinfunction "PE15")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 4 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 407 "QSPI_SS")
			(pinfunction "PB10")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 4.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 401 "unconnected-(U3-PB11-Pad47)")
			(pinfunction "PB11")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 383 "Net-(C145-Pad2)")
			(pinfunction "VCAP")
			(pintype "power_out")
		)
		(pad "49" smd roundrect
			(at 5.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "50" smd roundrect
			(at 6 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at 7.675 6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 356 "FPGA_CS")
			(pinfunction "PB12")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 7.675 5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 381 "FPGA_SCLK")
			(pinfunction "PB13")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 7.675 5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 290 "SDIO_DAT0")
			(pinfunction "PB14")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 7.675 4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 292 "SDIO_DAT1")
			(pinfunction "PB15")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 7.675 4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 447 "USER_PD8")
			(pinfunction "PD8")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at 7.675 3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 450 "USER_PD9")
			(pinfunction "PD9")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at 7.675 3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 446 "USER_PD10")
			(pinfunction "PD10")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at 7.675 2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 405 "FMC_A16")
			(pinfunction "PD11")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at 7.675 2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 412 "QSPI_SD1")
			(pinfunction "PD12")
			(pintype "bidirectional")
		)
		(pad "60" smd roundrect
			(at 7.675 1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 448 "USER_PD13")
			(pinfunction "PD13")
			(pintype "bidirectional")
		)
		(pad "61" smd roundrect
			(at 7.675 1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 400 "FMC_D0")
			(pinfunction "PD14")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at 7.675 0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 402 "FMC_D1")
			(pinfunction "PD15")
			(pintype "bidirectional")
		)
		(pad "63" smd roundrect
			(at 7.675 0 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 403 "unconnected-(U3-PC6-Pad63)")
			(pinfunction "PC6")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at 7.675 -0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 414 "FMC_NE1")
			(pinfunction "PC7")
			(pintype "bidirectional")
		)
		(pad "65" smd roundrect
			(at 7.675 -1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 399 "unconnected-(U3-PC8-Pad65)")
			(pinfunction "PC8")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at 7.675 -1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 420 "QSPI_SD0")
			(pinfunction "PC9")
			(pintype "bidirectional")
		)
		(pad "67" smd roundrect
			(at 7.675 -2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 404 "unconnected-(U3-PA8-Pad67)")
			(pinfunction "PA8")
			(pintype "bidirectional")
		)
		(pad "68" smd roundrect
			(at 7.675 -2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 455 "HPD_EN")
			(pinfunction "PA9")
			(pintype "bidirectional")
		)
		(pad "69" smd roundrect
			(at 7.675 -3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "TYPEC_ORI")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "70" smd roundrect
			(at 7.675 -3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "USB_DN")
			(pinfunction "PA11")
			(pintype "bidirectional")
		)
		(pad "71" smd roundrect
			(at 7.675 -4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 169 "USB_DP")
			(pinfunction "PA12")
			(pintype "bidirectional")
		)
		(pad "72" smd roundrect
			(at 7.675 -4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 136 "MCU_SWDIO")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "73" smd roundrect
			(at 7.675 -5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 383 "Net-(C145-Pad2)")
			(pinfunction "VCAP")
			(pintype "power_out")
		)
		(pad "74" smd roundrect
			(at 7.675 -5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "75" smd roundrect
			(at 7.675 -6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "76" smd roundrect
			(at 6 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 327 "MCU_SWCLK")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "77" smd roundrect
			(at 5.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "TCPC_INT")
			(pinfunction "PA15")
			(pintype "bidirectional")
		)
		(pad "78" smd roundrect
			(at 5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 331 "FPGA_PROG")
			(pinfunction "PC10")
			(pintype "bidirectional")
		)
		(pad "79" smd roundrect
			(at 4.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 333 "FPGA_DONE")
			(pinfunction "PC11")
			(pintype "bidirectional")
		)
		(pad "80" smd roundrect
			(at 4 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 332 "FPGA_SUSP")
			(pinfunction "PC12")
			(pintype "bidirectional")
		)
		(pad "81" smd roundrect
			(at 3.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 418 "FMC_D2")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "82" smd roundrect
			(at 3 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 416 "FMC_D3")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "83" smd roundrect
			(at 2.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 354 "EPD_THROT")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "84" smd roundrect
			(at 2 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "DP_PDN")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "85" smd roundrect
			(at 1.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 410 "FMC_NOE")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "86" smd roundrect
			(at 1 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 417 "FMC_NWE")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "87" smd roundrect
			(at 0.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 249 "DEC_RST")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "88" smd roundrect
			(at 0 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "DP_HPD")
			(pinfunction "PD7")
			(pintype "bidirectional")
		)
		(pad "89" smd roundrect
			(at -0.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 291 "SDIO_DAT2")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "90" smd roundrect
			(at -1 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 289 "SDIO_DAT3")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "91" smd roundrect
			(at -1.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "KEY2")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "92" smd roundrect
			(at -2 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "I2C1_SCL")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "93" smd roundrect
			(at -2.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "I2C1_SDA")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "94" smd roundrect
			(at -3 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 347 "KEY1")
			(pinfunction "BOOT0")
			(pintype "input")
		)
		(pad "95" smd roundrect
			(at -3.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 449 "USER_PB8")
			(pinfunction "PB8")
			(pintype "bidirectional")
		)
		(pad "96" smd roundrect
			(at -4 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 445 "USER_PB9")
			(pinfunction "PB9")
			(pintype "bidirectional")
		)
		(pad "97" smd roundrect
			(at -4.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 335 "/mcu/G_LED")
			(pinfunction "PE0")
			(pintype "bidirectional")
		)
		(pad "98" smd roundrect
			(at -5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 336 "/mcu/R_LED")
			(pinfunction "PE1")
			(pintype "bidirectional")
		)
		(pad "99" smd roundrect
			(at -5.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "100" smd roundrect
			(at -6 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-100_14x14mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 114.925 102.49 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -2.29 1.525 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U5-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 112 43.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C171"
			(at 0.2 3.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "VCOM_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 53.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C168"
			(at 9 2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 340 "VN_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.7 103.2 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 91.25 46.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R78"
			(at 1.05 3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "150K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25755"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "Net-(U23-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 98.85 37.6 180)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L12"
			(at -2.95 -0.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 459 "Net-(D17-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 112.18 52.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C146"
			(at 0.02 4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 383 "Net-(C145-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 80.95 53.6)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at -2.2 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 99.65 46)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C173"
			(at -3.4 -2.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "+5V_ES")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 103.68 69.94)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C207"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 87.9 104.6 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 1.6 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0006"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/fpga_ddr/DRAM_CKE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 85.4 104.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C72"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 124.08 38.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0.12 -4.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 365 "/mcu/OSC_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 134.32 102.8 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 0.4 -4.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M/1%"
			(at 0 1.17 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "Net-(U15-XTALN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "Net-(U15-XTALP)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.9375 49.35 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at -0.15 -0.97 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(Q2-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 82 40.5 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D3"
			(at 2.5 0.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.55 0.4 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 458 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0 180)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-6"
		(layer "F.Cu")
		(at 117.2875 86.6375)
		(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U20"
			(at -3.2875 -1.2375 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SY8113C"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6338414"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT*23*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 279 "Net-(U20-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "Net-(U20-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 280 "Net-(U20-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 74.1 62.1)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C62"
			(at 0 4.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "+VGH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 121.8 80.6 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C111"
			(at -0.4 1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 164 "/dp_in/SBU2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 163 "/dp_in/DPAUXP")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 54.35)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R115"
			(at 9.065 2.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 340 "VN_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_SOD-323_Alt"
		(layer "F.Cu")
		(at 106 37.4)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D5"
			(at -0.2 -2.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:D_SOD-323_Alt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C488405"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 294 "VCOM_DAC")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.2 0)
			(size 0.75 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 119.6 72.6 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C122"
			(at 0.6 -2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(at 68.5 33.5)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H4"
			(at 0 -2.9 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 2.9 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "DNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
			(remove_unused_layers no)
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 142.9 77.2 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0 -1.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C26083"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 324 "+VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "VBUS_MEA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 88.4 46)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 2 -8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 453 "/epd_power/+5V_VGH")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC"
		(layer "F.Cu")
		(at 151 52 -90)
		(descr "http://industrial.panasonic.com/cdbs/www-data/pdf/ATV0000/ATV0000CE5.pdf")
		(tags "SMD SMT SPST EVQPUL EVQPUC")
		(property "Reference" "SW3"
			(at 0 3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SW"
			(at 1.2 4.8 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Button_Switch_SMD:Panasonic_EVQPUL_EVQPUC"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C79174"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -1.375 90)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0 1.375 90)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu" "In8.Cu"
				"In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
				"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
				"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
				"In30.Cu"
			)
		)
		(pad "1" smd rect
			(at -2.625 -0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "KEY3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 2.625 -0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "KEY3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.625 0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.625 0.85 90)
			(size 1.55 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/EVQPU-LC-02K.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 74.1 63.15)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at 0 4.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 284 "-VCOM")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 90.8 93.1)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C79"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 141.3 69.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C140"
			(at 0 -2.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 310 "Net-(U13-VIN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 96.725 66)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 111.6 42.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R66"
			(at -0.1 1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25105"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "Net-(Q8-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 159 "VCOM_MEA_EN")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120.8 80.6 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C112"
			(at 0.6 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 162 "/dp_in/SBU1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "/dp_in/DPAUXN")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 135.4 74.6)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C98"
			(at -2.8 0.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 310 "Net-(U13-VIN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 93.25 34.8)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C167"
			(at -2.4 0.4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/50V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119903"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "+VP")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 124.62 96 180)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN13"
			(at 1.700001 0.149999 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R / 4D02WGF330JTCE"
			(at 0 2.1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C425299"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 275 "/tmds_in/ADV_P0")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 276 "/tmds_in/ADV_P1")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 277 "/tmds_in/ADV_P2")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 278 "/tmds_in/ADV_P3")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 243 "DPI_B3")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 244 "DPI_B2")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 180)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 345 "unconnected-(RN13-R2.2-Pad7)")
			(pinfunction "R2.2")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 180)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 346 "unconnected-(RN13-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 115.525 88.9 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C154"
			(at 2.325 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 307 "+1V8_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "Net-(U20-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 55.35 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R116"
			(at -9.065 -2.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 340 "VN_MEA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 56.4 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R118"
			(at -9.065 -2.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "VGL_MEA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 118.55 72.63 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C116"
			(at 0.63 -1.95 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 132.32 102.8 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C133"
			(at 0.9 -4.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Changjiang_FNR3012S"
		(layer "F.Cu")
		(at 93.25 39.6 180)
		(descr "Inductor, Changjiang, FNR3012S, 3.0x3.0x1.2mm, https://datasheet.lcsc.com/lcsc/1806131217_cjiang-Changjiang-Microelectronics-Tech-FNR5040S3R3NT_C167960.pdf")
		(tags "Inductor wirewound power shielded")
		(property "Reference" "L10"
			(at 2.4 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WPN3012H4R7MT"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_Changjiang_FNR3012S"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C98357"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 452 "/epd_power/+5V_VSH")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.15 0 180)
			(size 0.8 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "Net-(D15-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FNR3012S.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 110 103.4 90)
		(property "Reference" "H14"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.01 -0.01 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93.9 92.6 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C78"
			(at 2.2 0.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.6 39.85134 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C215"
			(at 0 1.05134 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 74.1 64.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C147"
			(at 0 4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 287 "+5V2_FL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 136.7 72.5 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C94"
			(at -3 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 308 "/power/EVDD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.4 48.2 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C172"
			(at -5.4 1.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 302 "+5V_ES")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 74.1 61.05)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C63"
			(at 0 4.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "-VGL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 86.6 92.4 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R101"
			(at 2.4 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0006"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/fpga_ddr/DRAM_CSB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.25 41.6 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C174"
			(at -1.6 0.75 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 459 "Net-(D17-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(U26-BS)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 86.9 104.6 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R102"
			(at 1.6 0.9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "240R/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25094"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0009"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 338 "Net-(U12-ZQ)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 138.78 102.02 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C114"
			(at 1.42 1.02 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 85.65 46.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at -1.75 -9.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "390K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25782"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U24-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "+VGH")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 110 67 90)
		(property "Reference" "H15"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.02 0 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 141.9 77.2 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 0.2 -2.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "VBUS_MEA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 73.775 84.75 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C159"
			(at 6.85 -0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 113.625 92.8875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 2.5 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 307 "+1V8_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 104.325 96.2)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R60"
			(at -2.8 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 285 "+1V2_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 105.5375 88.8)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C64"
			(at 2.0625 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.2 82.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.4 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "/dp_in/TX1N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "/dp_in/TX1NC")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 130.82 103.2 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C134"
			(at 3.4 1.22 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_1.27mm:PinSocket_2x06_P1.27mm_Vertical_SMD"
		(layer "F.Cu")
		(at 139 56 180)
		(descr "surface-mounted straight socket strip, 2x06, 1.27mm pitch, double cols (from Kicad 4.0.7!), script generated")
		(tags "Surface mounted socket strip SMD 2x06 1.27mm double row")
		(property "Reference" "J5"
			(at -4.4 1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2x6_1.27_HDR"
			(at 0 5.31 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinSocket_1.27mm:PinSocket_2x06_P1.27mm_Vertical_SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C3975132"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.8 -3.175 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "FPGA_TCK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.8 -3.175 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.8 -1.905 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "FPGA_TDI")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.8 -1.905 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.8 -0.635 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "FPGA_TDO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -1.8 -0.635 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.8 0.635 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "FPGA_TMS")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -1.8 0.635 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 1.8 1.905 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 327 "MCU_SWCLK")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -1.8 1.905 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 1.8 3.175 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 136 "MCU_SWDIO")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -1.8 3.175 180)
			(size 2.1 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 301 "+3V3")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_2x06_P1.27mm_Vertical_SMD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(layer "F.Cu")
		(at 142.8 79.8 180)
		(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
		(tags "UDFN-10 U-DFN2510-10 Diodes")
		(property "Reference" "D12"
			(at -1.6 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RCLAMP0524P"
			(at 0 2.54 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C907837"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "UDFN*1.0x3.8mm*P0.5mm*")
		(sheetname "dp_in")
		(sheetfile "dp_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "/dp_in/RX2P")
			(pinfunction "IO1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "/dp_in/RX2N")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.35 0 90)
			(size 0.45 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "/dp_in/TX2P")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "/dp_in/TX2N")
			(pinfunction "IO4")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.3875 1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "/dp_in/TX2N")
			(pinfunction "NC1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.3875 0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "/dp_in/TX2P")
			(pinfunction "NC2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.4125 0 90)
			(size 0.45 0.575)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.3875 -0.5 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "/dp_in/RX2N")
			(pinfunction "NC3")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.3875 -1 90)
			(size 0.25 0.625)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "/dp_in/RX2P")
			(pinfunction "NC4")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 80.05 45.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 2.05 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U9-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 85.65 45.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at -1.75 -9.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U24-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "+VGH")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 89.4 104.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C74"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_BGA:WLP-4_0.83x0.83mm_P0.4mm"
		(layer "F.Cu")
		(at 87.7 49 180)
		(descr "WLP-4_0.83x0.83mm_P0.4mm https://pdfserv.maximintegrated.com/package_dwgs/21-100107.PDF, https://www.maximintegrated.com/en/app-notes/index.mvp/id/1891")
		(tags "WLP-4")
		(property "Reference" "U8"
			(at 1.4 0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS22914BYFPR"
			(at 0 2.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_BGA:WLP-4_0.83x0.83mm_P0.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP22913.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Slew rate controlled load switch, WLCSP-4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C1848394"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WLCSP*X1*WLB0909*0.89x0.89*P0.5mm*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -0.2 -0.2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 453 "/epd_power/+5V_VGH")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "A2" smd circle
			(at 0.2 -0.2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 303 "+5V_EG")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "B1" smd circle
			(at -0.2 0.2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B2" smd circle
			(at 0.2 0.2 180)
			(size 0.25 0.25)
			(property pad_prop_bga)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 221 "EPD_POS_EN")
			(pinfunction "ON")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_BGA.3dshapes/WLP-4_0.83x0.83mm_P0.4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 85.65 47.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 1.75 9.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25768"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "Net-(U24-FB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-6"
		(layer "F.Cu")
		(at 104.7 86.6)
		(descr "TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U28"
			(at -1.2 2.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SY8113C"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6338414"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT*23*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U28-BS)")
			(pinfunction "BS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U28-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U28-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.075 39.15 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0.475 3.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U11-+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 139.5 66.2 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C96"
			(at -0.1 3.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 439 "+5V_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 73.775 82.775 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at -6.225 0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd")
		(sheetfile "epd.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120.4 36 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 2 -0.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18pF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C106202"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 366 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 96.85 47.6 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R89"
			(at -2.05 -0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25768"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "-VN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(U26-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:ICSRC6508-030SFR"
		(layer "F.Cu")
		(at 76 85.55 90)
		(property "Reference" "H26"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ICSRC6508-030SFR"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "footprints:ICSRC6508-030SFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C2836609"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "pcb.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.01 0.12 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0 0 90)
			(size 1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 2.75 0 90)
			(size 1.1 0.8)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at 0 0 90)
			(size 6.7 0.9)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/ICSRC6508-030SFR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 145.3 48.38 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D20"
			(at 0 -1.29 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED RED"
			(at 0 1.43 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C965799"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D20-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 122.1 38.4 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at -0.1 4.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 379 "/mcu/OSC_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 366 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 141.6 99.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100R/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.001"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25076"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 451 "Net-(U15-HPA_A{slash}INT2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 222 "/tmds_in/HDMI_HPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.02 39.15)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C160"
			(at -0.22 -3.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 141.52 91.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C132"
			(at -1.12 -2.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 1.16 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 112.775 54.725 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 4.075 -0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.21 44.65 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at -0.01 -3.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25744"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 347 "KEY1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 111.6 45.6 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R63"
			(at 0 -1.17 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33R/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25105"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 158 "VCOM_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "Net-(Q7-G)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.9375 53.35 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at -0.05 0.9375 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 116.9 38.08 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 1.88 -0.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 374 "+3V3A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 142.6 48.4)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 0 1.07 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1K/1%"
			(at 0 1.17 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 336 "/mcu/R_LED")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D20-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93 57.1 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C143"
			(at 1.5 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 299 "+3V3_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 101 86.7 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R57"
			(at -0.1 2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100K/1%"
			(at 0 1.17 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C25741"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 285 "+1V2_DCDC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U28-FB)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 121.225 93 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R72"
			(at -2.6 -0.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20mR"
			(at 0 1.65 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C7467301"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "power_mon")
		(sheetfile "power_mon.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 287 "+5V2_FL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 439 "+5V_DCDC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm"
		(layer "F.Cu")
		(at 108.295 52.3 -90)
		(descr "WSON, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf (page 68)), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "WSON NoLead")
		(property "Reference" "U14"
			(at -0.1 3.295 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q32JV"
			(at 0 3.45 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C571260"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.9559"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WSON*1EP*6x5mm*P1.27mm*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.85 -1.075 270)
			(size 1.37 1.73)
			(layers "F.Paste")
			(roundrect_rratio 0.182482)
		)
		(pad "" smd roundrect
			(at -0.85 1.075 270)
			(size 1.37 1.73)
			(layers "F.Paste")
			(roundrect_rratio 0.182482)
		)
		(pad "" smd roundrect
			(at 0.85 -1.075 270)
			(size 1.37 1.73)
			(layers "F.Paste")
			(roundrect_rratio 0.182482)
		)
		(pad "" smd roundrect
			(at 0.85 1.075 270)
			(size 1.37 1.73)
			(layers "F.Paste")
			(roundrect_rratio 0.182482)
		)
		(pad "1" smd roundrect
			(at -2.7 -1.905 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 407 "QSPI_SS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.7 -0.635 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 412 "QSPI_SD1")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.7 0.635 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 419 "QSPI_SD2")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.7 1.905 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.7 1.905 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 420 "QSPI_SD0")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.7 0.635 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 316 "QSPI_SCLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.7 -0.635 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 409 "QSPI_SD3")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.7 -1.905 270)
			(size 0.75 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 3.4 4.3)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 315 "GND")
			(pinfunction "EP")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.6 37.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 2.1 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 1.16 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 136.6 42.2 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C214"
			(at 0 1.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "mcu")
		(sheetfile "mcu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 80.95 51.6)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at -3.15 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/10V"
			(at 0 1.68 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" " C29277"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "epd_power")
		(sheetfile "epd_power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V_EPD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 89.48 76.401)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at 24.4 -0.051 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 93.5 76.9 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at -0.05 -24.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 84.4 80.8)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R103"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "5.1K/1%"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C25905"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0006"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 54 "/fpga_ddr/DRAM_RST")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 91.48 76.401 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C68"
			(at -24.42 0.051 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 100.125 80.9)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C92"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 84.5 103.1)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R104"
			(at 17.9 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1K/1%"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0025"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 138.62 95.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C130"
			(at 2.450001 0.050001 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 -1.16 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 98.2 77)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C150"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 85.4 104.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C87"
			(at 18.3 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0165"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 95.7 102.2 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C81"
			(at -0.1 -18.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 95.46 81.301)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C189"
			(at 24.4 -0.051 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 90.5 72.225 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0.05 24.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 87.725 77.9 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at -24.4 0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 86.7 98.7 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R100"
			(at 0.1 18.3 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100R/1%"
			(at 0 -1.17 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C25076"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.001"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/fpga_ddr/DRAM_CKN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 9 "/fpga_ddr/DRAM_CKP")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 84.36 83.401 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C157"
			(at -24.4 0.051 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 83.625 70.9)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C156"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 85.22 77.95)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C188"
			(at 24.4 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 85.08 68.1 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C182"
			(at -24.4 0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 95.51 78.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 24.39 0.65 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100R/1%"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C25076"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0007"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 334 "Net-(U1D-IO_L1P_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 138.62 98.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C138"
			(at 2.450001 0.150001 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 -1.16 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 305 "+1V8_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 86.5 102.1)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C144"
			(at 18.5 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0023"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 89 72.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0.05 24.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 79.88 81.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C70"
			(at -24.42 0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 94.98 75.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C183"
			(at 23.82 -0.4 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 97.1 72.95 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C93"
			(at -24.4 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 92.8 73)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 95.3 77.1 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C190"
			(at -0.25 24.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 97.5 81.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0.05 24.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 96.32 71.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C187"
			(at -24.4 0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 80.52 79.8 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C184"
			(at -24.4 0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 90.5 69.175 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C149"
			(at 0.05 24.4 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 87.45 71.1 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0.05 24.45 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 85 100.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C76"
			(at 18.3 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 95 95.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C83"
			(at 0.1 18.3 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 97 102.4 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C86"
			(at -0.1 -18.3 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0301"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 89.2 101.3 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C84"
			(at -0.1 -18.3 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 89.5 74.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 89.48 75.401)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 24.4 -0.051 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 138.62 94.1 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C129"
			(at 2.450001 0.050001 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 -1.16 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 137.2 100.8 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C162"
			(at 0 1.43 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6.3V"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C59461"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 138.62 97.1 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C126"
			(at 2.450001 0.050001 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "tmds_in")
		(sheetfile "tmds_in.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 306 "+3V3_VID")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 91.48 75.401 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at -24.42 0.051 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 60 "+1V2_FPGA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 91.5 74.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 24.4 -0.05 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/6.3V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C307423"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "power")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 301 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 84.5 102.1)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C88"
			(at 18.2 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF/50V"
			(at 0 -1.16 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C131394"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0023"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 86.5 103.1)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R105"
			(at 18.5 -0.1 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1K/1%"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C11702"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0025"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "fpga_ddr")
		(sheetfile "fpga_ddr.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+DRAM_VREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 93.2 78.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C185"
			(at -0.4 24.42 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/25V"
			(at 0 -1.16 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LCSC" "C6119801"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.0036"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "desc" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "fpga_config")
		(sheetfile "fpga_config.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 304 "+1V35")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 315 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 149.8 95.25)
		(end 149.8 106.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.7 30)
		(end 151 30)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154 48)
		(end 154 33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 106.75)
		(end 155 107)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 68.7 110)
		(mid 66.083705 108.916295)
		(end 65 106.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.8 106.75)
		(end 155 106.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 95.25)
		(end 149.8 95.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 65 33.7)
		(end 65 106.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 78)
		(end 155 80.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150 89.55)
		(end 155 89.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.7 110)
		(end 152 110)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 65 33.7)
		(mid 66.083705 31.083705)
		(end 68.7 30)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153 78)
		(end 153 48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150 80.25)
		(end 150 89.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153 48)
		(end 154 48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 78)
		(end 153 78)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 155 107)
		(mid 154.12132 109.12132)
		(end 152 110)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 151 30)
		(mid 153.12132 30.87868)
		(end 154 33)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 89.55)
		(end 155 95.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155 80.25)
		(end 150 80.25)
		(layer "Edge.Cuts")
	)
	(gr_text "VGL"
		(at 81 33.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "PB8"
		(at 71.6 51.4 0)
		(layer "F.SilkS")
	)
	(gr_text "VN"
		(at 98.2 33.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "VCOM"
		(at 109.3 35.3 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "VGH"
		(at 86.4 33.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Glider"
		(at 71 34.7 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 71.6 38.6 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO"
		(at 67.5 37 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "VP"
		(at 92.6 33.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "EPD1"
		(at 67.5 58.3 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "EPD2"
		(at 67.5 89.8 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "250908"
		(at 71.2 107.4 0)
		(layer "F.SilkS")
	)
	(gr_text "PB9"
		(at 71.6 53.8 0)
		(layer "F.SilkS")
	)
	(gr_text "PD13"
		(at 71.6 48.8 0)
		(layer "F.SilkS")
	)
	(gr_text "JTAG"
		(at 144.2 55.2 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "PD9"
		(at 71.6 43.6 0)
		(layer "F.SilkS")
	)
	(gr_text "Modos"
		(at 71.1 33.2 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 71.6 56.4 0)
		(layer "F.SilkS")
	)
	(gr_text "PD8"
		(at 71.6 41.2 0)
		(layer "F.SilkS")
	)
	(gr_text "R1.3"
		(at 71.2 106.4 0)
		(layer "F.SilkS")
	)
	(gr_text "PD10"
		(at 71.6 46.2 0)
		(layer "F.SilkS")
	)
	(gr_text "U13"
		(at 136.1 69.1 90)
		(layer "F.Fab")
	)
	(gr_text "C60"
		(at 73.9 83.09 90)
		(layer "F.Fab")
	)
	(zone
		(net 301)
		(net_name "+3V3")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.11)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64 29) (xy 64 111) (xy 156 111) (xy 156 29)
			)
		)
	)
	(zone
		(net 60)
		(net_name "+1V2_FPGA")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.11)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104 97) (xy 102 97) (xy 102 95) (xy 104 93) (xy 104 81) (xy 99.5 76.5) (xy 90.25 76.5) (xy 89.75 77)
				(xy 89 77) (xy 88 76) (xy 88 75) (xy 88.75 74.25) (xy 91.5 74.25) (xy 92 73.75) (xy 92.75 73.75)
				(xy 93 74) (xy 93 75.25) (xy 93.25 75.5) (xy 102 75.5) (xy 106.25 79.75) (xy 106.25 94.75)
			)
		)
	)
	(zone
		(net 304)
		(net_name "+1V35")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.11)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 76 83) (xy 76 101) (xy 80 105) (xy 98 105) (xy 100.75 102.25) (xy 100.75 92.75) (xy 102 91.5)
				(xy 102 88) (xy 100 86) (xy 100 82) (xy 97 79) (xy 94 79) (xy 93 78) (xy 84 78) (xy 81 81) (xy 78 81)
			)
		)
	)
	(zone
		(net 324)
		(net_name "+VBUS")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.11)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.8 74) (xy 142.8 76.1) (xy 144.2 77.7) (xy 145.4 77.7) (xy 145.4 86.1) (xy 145.9 86.7) (xy 147.2 86.7)
				(xy 147.7 86.2) (xy 147.7 77.4) (xy 143.9 73.6) (xy 143.2 73.6)
			)
		)
	)
	(zone
		(net 315)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.11)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64 29.2) (xy 64 111.2) (xy 156 111.2) (xy 156 29.2)
			)
		)
	)
)
