(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "glider_mega_adapter")
		(date "2025-10-22")
		(rev "r0.1")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3V3")
	(net 3 "/GDOE")
	(net 4 "/GDCLK")
	(net 5 "/GDSP")
	(net 6 "/ESDCLK")
	(net 7 "/ED0")
	(net 8 "/ED8")
	(net 9 "/ED1")
	(net 10 "/ED9")
	(net 11 "/ED2")
	(net 12 "/ED10")
	(net 13 "/ED3")
	(net 14 "/ED11")
	(net 15 "/ED4")
	(net 16 "/ED12")
	(net 17 "/ED5")
	(net 18 "/ED13")
	(net 19 "/ED6")
	(net 20 "/ED14")
	(net 21 "/ED7")
	(net 22 "/ED15")
	(net 23 "/SDCE0")
	(net 24 "/ESDLE")
	(net 25 "/ESDOE")
	(net 26 "unconnected-(J1-Pin_2-Pad2)")
	(net 27 "-VGL")
	(net 28 "-VCOM")
	(net 29 "unconnected-(J1-Pin_4-Pad4)")
	(net 30 "unconnected-(J1-Pin_34-Pad34)")
	(net 31 "+VP")
	(net 32 "unconnected-(J1-Pin_39-Pad39)")
	(net 33 "-VN")
	(net 34 "unconnected-(J1-Pin_37-Pad37)")
	(net 35 "+VGH")
	(net 36 "unconnected-(J1-Pin_35-Pad35)")
	(net 37 "unconnected-(J3-Pin_44-Pad44)")
	(net 38 "unconnected-(J3-Pin_42-Pad42)")
	(net 39 "unconnected-(J3-Pin_41-Pad41)")
	(net 40 "unconnected-(J3-Pin_7-Pad7)")
	(net 41 "unconnected-(J3-Pin_4-Pad4)")
	(net 42 "unconnected-(J3-Pin_43-Pad43)")
	(net 43 "unconnected-(J3-Pin_50-Pad50)")
	(net 44 "unconnected-(J3-Pin_2-Pad2)")
	(net 45 "unconnected-(J3-Pin_48-Pad48)")
	(net 46 "unconnected-(J3-Pin_46-Pad46)")
	(net 47 "unconnected-(J4-Pin_2-Pad2)")
	(net 48 "unconnected-(J4-Pin_27-Pad27)")
	(net 49 "/UD")
	(net 50 "unconnected-(J4-Pin_21-Pad21)")
	(net 51 "unconnected-(J4-Pin_25-Pad25)")
	(net 52 "unconnected-(J4-Pin_6-Pad6)")
	(net 53 "unconnected-(J4-Pin_23-Pad23)")
	(net 54 "unconnected-(J4-Pin_4-Pad4)")
	(net 55 "/RL")
	(net 56 "unconnected-(J5-Pin_5-Pad5)")
	(net 57 "unconnected-(J5-Pin_23-Pad23)")
	(net 58 "unconnected-(J5-Pin_24-Pad24)")
	(net 59 "unconnected-(J5-Pin_30-Pad30)")
	(net 60 "unconnected-(J5-Pin_4-Pad4)")
	(net 61 "unconnected-(J5-Pin_25-Pad25)")
	(net 62 "unconnected-(J5-Pin_22-Pad22)")
	(net 63 "unconnected-(J6-Pin_10-Pad10)")
	(net 64 "Net-(J6-Pin_30)")
	(net 65 "unconnected-(J6-Pin_25-Pad25)")
	(net 66 "unconnected-(J6-Pin_21-Pad21)")
	(net 67 "unconnected-(J6-Pin_27-Pad27)")
	(net 68 "unconnected-(J6-Pin_26-Pad26)")
	(net 69 "unconnected-(RN2-R2.1-Pad2)")
	(net 70 "unconnected-(RN2-R2.2-Pad7)")
	(net 71 "/PD8")
	(net 72 "/PD12")
	(net 73 "/PSDLE")
	(net 74 "/PGDOE")
	(net 75 "/PSDCE0")
	(net 76 "/PD5")
	(net 77 "/PD9")
	(net 78 "/PD11")
	(net 79 "/PD3")
	(net 80 "/PD0")
	(net 81 "/PGDSP")
	(net 82 "/PD14")
	(net 83 "/PD15")
	(net 84 "/PD13")
	(net 85 "/PSDOE")
	(net 86 "/PD1")
	(net 87 "/PD2")
	(net 88 "/PD10")
	(net 89 "/PSDCLK")
	(net 90 "/PGDCLK")
	(net 91 "/PD7")
	(net 92 "/PD4")
	(net 93 "/PD6")
	(net 94 "/SPI_SCLK")
	(net 95 "/SPI_MISO")
	(net 96 "/SPI_VDD")
	(net 97 "/SPI_MOSI")
	(net 98 "unconnected-(J9-Pin_8-Pad8)")
	(net 99 "unconnected-(J9-Pin_7-Pad7)")
	(net 100 "Net-(J9-Pin_10)")
	(net 101 "/SPI_NCS")
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 170.75 84 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN4"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/PD8")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "/PD9")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "/PD10")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "/PD11")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/ED11")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/ED10")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/ED9")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/ED8")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Xunpu_FPC-05F-50PH20_1x50-1MP_P0.50mm_Horizontal_Mirrored"
		(layer "F.Cu")
		(at 170.5 88.5)
		(descr "Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
		(tags "connector Hirose FH12 horizontal")
		(property "Reference" "J3"
			(at 0 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "FH12-50S-0.5SH"
			(at 0 5.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:Xunpu_FPC-05F-50PH20_1x50-1MP_P0.50mm_Horizontal_Mirrored"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "\"Generic connectable mounting pin connector, single row, 01x50, script generated\""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 12.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "-VGL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 11.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "unconnected-(J3-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at 11.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "+VGH")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 10.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "unconnected-(J3-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at 10.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 9.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 9.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "unconnected-(J3-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 8.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "/PSDOE")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 8.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "/PSDLE")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 7.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "/PSDCE0")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 7.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "/PGDOE")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 6.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/PGDSP")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 6.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "/PGDCLK")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 5.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 5.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "/PSDCLK")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 4.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 4.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "/PD15")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 3.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "/PD14")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 3.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 2.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "/PD13")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 2.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "/PD12")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 1.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 1.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "/PD11")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 0.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "/PD10")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 0.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at -0.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "/PD9")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at -0.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/PD8")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at -1.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -1.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "/PD7")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -2.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "/PD6")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -2.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at -3.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "/PD5")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at -3.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "/PD4")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at -4.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at -4.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "/PD3")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at -5.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "/PD2")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -5.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at -6.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "/PD1")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -6.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "/PD0")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at -7.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at -7.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "unconnected-(J3-Pin_41-Pad41)")
			(pinfunction "Pin_41")
			(pintype "passive+no_connect")
		)
		(pad "42" smd rect
			(at -8.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "unconnected-(J3-Pin_42-Pad42)")
			(pinfunction "Pin_42")
			(pintype "passive+no_connect")
		)
		(pad "43" smd rect
			(at -8.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "unconnected-(J3-Pin_43-Pad43)")
			(pinfunction "Pin_43")
			(pintype "passive+no_connect")
		)
		(pad "44" smd rect
			(at -9.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "unconnected-(J3-Pin_44-Pad44)")
			(pinfunction "Pin_44")
			(pintype "passive+no_connect")
		)
		(pad "45" smd rect
			(at -9.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_45")
			(pintype "passive")
		)
		(pad "46" smd rect
			(at -10.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "unconnected-(J3-Pin_46-Pad46)")
			(pinfunction "Pin_46")
			(pintype "passive+no_connect")
		)
		(pad "47" smd rect
			(at -10.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_47")
			(pintype "passive")
		)
		(pad "48" smd rect
			(at -11.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "unconnected-(J3-Pin_48-Pad48)")
			(pinfunction "Pin_48")
			(pintype "passive+no_connect")
		)
		(pad "49" smd rect
			(at -11.75 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_49")
			(pintype "passive")
		)
		(pad "50" smd rect
			(at -12.25 -1.95 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "unconnected-(J3-Pin_50-Pad50)")
			(pinfunction "Pin_50")
			(pintype "passive+no_connect")
		)
		(pad "MP" smd rect
			(at -13.94 0.75)
			(size 1.8 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 13.94 0.75)
			(size 2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FPC-SMD_50P-P0.50_FPC-05F-50PH20.step"
			(offset
				(xyz 0 1.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 190 85)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "Net-(J9-Pin_10)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 165.1 84 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN6"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "/PD0")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "/PD1")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "/PD2")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "/PD3")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/ED3")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/ED2")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/ED1")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/ED0")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:Omron_XF2M-4015-1A_1x40-1MP_P0.5mm_Horizontal"
		(layer "F.Cu")
		(at 163 57 180)
		(descr "Omron FPC connector, 40 top-side contacts, 0.5mm pitch, SMT, https://omronfs.omron.com/en_US/ecb/products/pdf/en-xf2m.pdf")
		(tags "omron fpc xf2m")
		(property "Reference" "J1"
			(at 0 -3.7 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AFC24-S40FIA-00"
			(at 0 5.1 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_FFC-FPC:Omron_XF2M-4015-1A_1x40-1MP_P0.5mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -9.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "-VGL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -9.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -8.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "+VGH")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -8.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "unconnected-(J1-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -7.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -7.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -6.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GDCLK")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -6.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/GDSP")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -5.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -5.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -4.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -4.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -3.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/ESDCLK")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -3.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/ED0")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -2.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/ED1")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -2.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/ED2")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -1.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/ED3")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -1.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/ED4")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -0.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/ED5")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -0.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/ED6")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 0.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/ED7")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 0.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 1.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/ED8")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 1.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/ED9")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 2.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/ED10")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 2.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/ED11")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 3.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/ED12")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 3.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/ED13")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 4.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/ED14")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 4.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/ED15")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 5.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/SDCE0")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 5.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/ESDLE")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 6.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/ESDOE")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 6.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "unconnected-(J1-Pin_34-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive+no_connect")
		)
		(pad "35" smd rect
			(at 7.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "unconnected-(J1-Pin_35-Pad35)")
			(pinfunction "Pin_35")
			(pintype "passive+no_connect")
		)
		(pad "36" smd rect
			(at 7.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at 8.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "unconnected-(J1-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
		)
		(pad "38" smd rect
			(at 8.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at 9.25 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "unconnected-(J1-Pin_39-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive+no_connect")
		)
		(pad "40" smd rect
			(at 9.75 -2.05 180)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -11.4 1.85 180)
			(size 1.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 11.4 1.85 180)
			(size 1.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "/Users/wenting/Documents/projects/GliderPrivate/pcb/pcb_common/footprints.pretty/XF2M-4015-1A.STEP"
			(offset
				(xyz 0 -3 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150.7 71 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.17 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/UD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 178.75 84 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN1"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "/PGDOE")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "/PSDCE0")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "/PSDLE")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "/PSDOE")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/ESDOE")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/ESDLE")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/SDCE0")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 173.5 84 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN3"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "/PD12")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 84 "/PD13")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "/PD14")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "/PD15")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/ED15")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/ED14")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/ED13")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/ED12")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150 83.3 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(J6-Pin_30)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 176.1 84 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN2"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "/PSDCLK")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "unconnected-(RN2-R2.1-Pad2)")
			(pinfunction "R2.1")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "/PGDCLK")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/PGDSP")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/GDSP")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GDCLK")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "unconnected-(RN2-R2.2-Pad7)")
			(pinfunction "R2.2")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/ESDCLK")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Array_Convex_4x0402"
		(layer "F.Cu")
		(at 167.95 84 90)
		(descr "Chip Resistor Network, ROHM MNR04 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "RN5"
			(at 1.6 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_Array_Convex_4x0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "/PD4")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "/PD5")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "/PD6")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "/PD7")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.5 0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/ED7")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.5 0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/ED6")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 -0.25 90)
			(size 0.5 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/ED5")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.5 -0.75 90)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/ED4")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0402.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Xunpu_FPC-05F-50PH20_1x50-1MP_P0.50mm_Horizontal"
		(layer "F.Cu")
		(at 195 77 90)
		(descr "Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
		(tags "connector Hirose FH12 horizontal")
		(property "Reference" "J9"
			(at 0 -3.7 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FH28-50S-0.5SH"
			(at 0 5.6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:Xunpu_FPC-05F-50PH20_1x50-1MP_P0.50mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "\"Generic connectable mounting pin connector, single row, 01x50, script generated\""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 3.7 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -12.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "/SPI_MISO")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -11.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "/SPI_MOSI")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -11.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "/SPI_NCS")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -10.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "/SPI_SCLK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -10.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 96 "/SPI_VDD")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -9.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -9.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "unconnected-(J9-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at -8.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "unconnected-(J9-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -8.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -7.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 100 "Net-(J9-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -7.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GDCLK")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -6.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/GDSP")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -6.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -5.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "+VGH")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -5.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -4.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "-VGL")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -4.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -3.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/ESDOE")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -3.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/ESDLE")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -2.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/SDCE0")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at -2.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -1.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/ED15")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -1.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/ED14")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -0.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/ED13")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -0.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/ED12")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 0.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/ED11")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 0.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/ED10")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 1.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/ED9")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 1.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/ED8")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 2.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 2.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/ESDCLK")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 3.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 3.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/ED7")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 4.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/ED6")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at 4.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/ED5")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 5.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/ED4")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at 5.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/ED3")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at 6.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/ED2")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at 6.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/ED1")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at 7.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/ED0")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at 7.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_41")
			(pintype "passive")
		)
		(pad "42" smd rect
			(at 8.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_42")
			(pintype "passive")
		)
		(pad "43" smd rect
			(at 8.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_43")
			(pintype "passive")
		)
		(pad "44" smd rect
			(at 9.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_44")
			(pintype "passive")
		)
		(pad "45" smd rect
			(at 9.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_45")
			(pintype "passive")
		)
		(pad "46" smd rect
			(at 10.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_46")
			(pintype "passive")
		)
		(pad "47" smd rect
			(at 10.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_47")
			(pintype "passive")
		)
		(pad "48" smd rect
			(at 11.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_48")
			(pintype "passive")
		)
		(pad "49" smd rect
			(at 11.75 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_49")
			(pintype "passive")
		)
		(pad "50" smd rect
			(at 12.25 -1.85 90)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_50")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -13.94 0.75 90)
			(size 1.8 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 13.94 0.75 90)
			(size 2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FPC-SMD_50P-P0.50_FPC-05F-50PH20.step"
			(offset
				(xyz 0 1.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 150.9 61.5 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -1.9 -0.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/RL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Molex_5025983993"
		(layer "F.Cu")
		(at 146 86.3 -90)
		(property "Reference" "J6"
			(at -0.1 -2.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "502598-3993"
			(at 8.64 3.265 90)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:Molex_5025983993"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "609-10064555-392120HLFCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ref.Price" "0.95"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 5.7 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 5.4 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 5.1 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 4.8 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 4.5 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/ESDCLK")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 4.2 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/ESDLE")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 3.9 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/ESDOE")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 3.6 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 3.3 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 3 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "unconnected-(J6-Pin_10-Pad10)")
			(pinfunction "Pin_10")
			(pintype "passive+no_connect")
		)
		(pad "11" smd rect
			(at 2.7 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/SDCE0")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 2.4 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/ED0")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 2.1 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/ED1")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.8 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/ED2")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.5 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/ED3")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 1.2 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/ED4")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0.9 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/ED5")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 0.6 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/ED6")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 0.3 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/ED7")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 0 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at -0.3 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "unconnected-(J6-Pin_21-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive+no_connect")
		)
		(pad "22" smd rect
			(at -0.6 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -0.9 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "+VGH")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -1.2 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "-VGL")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -1.5 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "unconnected-(J6-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
		)
		(pad "26" smd rect
			(at -1.8 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "unconnected-(J6-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
		)
		(pad "27" smd rect
			(at -2.1 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "unconnected-(J6-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
		)
		(pad "28" smd rect
			(at -2.4 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -2.7 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -3 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(J6-Pin_30)")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -3.3 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at -3.6 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/GDSP")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at -3.9 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GDCLK")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at -4.2 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at -4.5 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at -4.8 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -5.1 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at -5.4 -1.6 90)
			(size 0.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -5.7 1.4 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "S1" smd rect
			(at -6.675 1.125 270)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "S2" smd rect
			(at 6.675 1.125 270)
			(size 0.4 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FH26W-39S-0.3SHW.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Xunpu_FPC-05F-33PH20_1x33-1MP_P0.50mm_Horizontal"
		(layer "F.Cu")
		(at 146.35 64.5 -90)
		(descr "Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
		(tags "connector Hirose FH12 horizontal")
		(property "Reference" "J4"
			(at 0 -3.7 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FPC-05F-33PH20"
			(at 0 5.6 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:Xunpu_FPC-05F-33PH20_1x33-1MP_P0.50mm_Horizontal"
			(at 4.25 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 4.25 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x33, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 4.25 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 3.7 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "unconnected-(J4-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -7 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -6.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "unconnected-(J4-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -6 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -5.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "unconnected-(J4-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -4.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/ESDCLK")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -4 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/ESDLE")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -3.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/ESDOE")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -3 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/RL")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -2.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/SDCE0")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -2 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/ED0")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -1.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/ED1")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -1 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/ED2")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -0.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/ED3")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/ED4")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 0.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/ED5")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 1 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/ED6")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 1.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/ED7")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 2 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "unconnected-(J4-Pin_21-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive+no_connect")
		)
		(pad "22" smd rect
			(at 2.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 3 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "unconnected-(J4-Pin_23-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
		)
		(pad "24" smd rect
			(at 3.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "+VGH")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 4 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "unconnected-(J4-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
		)
		(pad "26" smd rect
			(at 4.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "-VGL")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "unconnected-(J4-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
		)
		(pad "28" smd rect
			(at 5.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 6 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 6.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/UD")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 7 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/GDSP")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 7.5 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GDCLK")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 8 -1.85 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -9.69 0.75 270)
			(size 1.8 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at 9.7 0.75 270)
			(size 2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FPC-SMD_F0502-B-34-15T-R.step"
			(offset
				(xyz 0 -0.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Hirose_FH34SRJ-34S-0.5SH_1x34-1MP_P0.50mm_Horizontal"
		(layer "F.Cu")
		(at 188.25 57.55 180)
		(property "Reference" "J5"
			(at 0 1.95 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FH34SRJ-34S-0.5SH"
			(at 0 3.1 180)
			(layer "F.Fab")
		)
		(property "Footprint" "footprints:Hirose_FH34SRJ-34S-0.5SH_1x34-1MP_P0.50mm_Horizontal"
			(at 1.5 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 1.5 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 1.5 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "adapter.kicad_sch")
		(attr smd)
		(pad "0" smd rect
			(at -9.375 3.3 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "0" smd rect
			(at 9.375 3.3 180)
			(size 0.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at -8.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "-VN")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -7.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "-VGL")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -7.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -6.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "unconnected-(J5-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -6.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "unconnected-(J5-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at -5.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "+3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at -5.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at -4.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/ESDCLK")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at -4.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at -3.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/ESDLE")
			(pinfunction "Pin_10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd rect
			(at -3.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "/ESDOE")
			(pinfunction "Pin_11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd rect
			(at -2.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/SDCE0")
			(pinfunction "Pin_12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd rect
			(at -2.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/ED0")
			(pinfunction "Pin_13")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd rect
			(at -1.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/ED1")
			(pinfunction "Pin_14")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "15" smd rect
			(at -1.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/ED2")
			(pinfunction "Pin_15")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "16" smd rect
			(at -0.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/ED3")
			(pinfunction "Pin_16")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "17" smd rect
			(at -0.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/ED4")
			(pinfunction "Pin_17")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "18" smd rect
			(at 0.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/ED5")
			(pinfunction "Pin_18")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "19" smd rect
			(at 0.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/ED6")
			(pinfunction "Pin_19")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "20" smd rect
			(at 1.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "/ED7")
			(pinfunction "Pin_20")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "21" smd rect
			(at 1.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_21")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "22" smd rect
			(at 2.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "unconnected-(J5-Pin_22-Pad22)")
			(pinfunction "Pin_22")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "23" smd rect
			(at 2.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "unconnected-(J5-Pin_23-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "24" smd rect
			(at 3.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "unconnected-(J5-Pin_24-Pad24)")
			(pinfunction "Pin_24")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "25" smd rect
			(at 3.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "unconnected-(J5-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "26" smd rect
			(at 4.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_26")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "27" smd rect
			(at 4.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GDOE")
			(pinfunction "Pin_27")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "28" smd rect
			(at 5.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/GDCLK")
			(pinfunction "Pin_28")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "29" smd rect
			(at 5.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/GDSP")
			(pinfunction "Pin_29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "30" smd rect
			(at 6.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "unconnected-(J5-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "31" smd rect
			(at 6.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "-VCOM")
			(pinfunction "Pin_31")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "32" smd rect
			(at 7.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "Pin_32")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "33" smd rect
			(at 7.75 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "+VP")
			(pinfunction "Pin_33")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "34" smd rect
			(at 8.25 0.4 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "+VGH")
			(pinfunction "Pin_34")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KIPRJMOD}/../pcb_common/footprints.pretty/FH34SRJ-40S-0.5SH.stp"
			(offset
				(xyz 0 -1.7 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 141 53)
		(end 200 93.9)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "40P-A/B"
		(at 157.6 63.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Contact facing down!"
		(at 180.4 59.4 0)
		(layer "F.SilkS")
	)
	(gr_text "34P-A"
		(at 178.4 63.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "39P-A"
		(at 151.6 91.8 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "50P-A"
		(at 190.2 80.8 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GLIDER MEGA ADAPTER\nREV 0.1"
		(at 170.2 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "33P-A"
		(at 152.6 70.2 90)
		(layer "F.SilkS" knockout)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 201 98) (xy 140 98) (xy 140 52) (xy 201 52)
			)
		)
	)
)
